| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLORAWAN_McastData Struct Reference

Structure containing a MultiCast Data. More...

`#include <SAP/WiMOD_SAP_LORAWAN_ProLink_IDs.h>`

## Public Attributes
UINT8 | StatusFormat
UINT32 | DeviceAddress
UINT8 | LoRaWANPort
UINT8 | AppPayload [WiMODLORAWAN_APP_PAYLOAD_LEN]
UINT8 | Length
UINT8 | ChannelIndex
UINT8 | DataRateIndex
INT8 | RSSI
INT8 | SNR
UINT8 | RxSlot
bool | OptionalInfoAvaiable

## Detailed Description

Structure containing a MultiCast Data.

## Member Data Documentation

## ◆ AppPayload

UINT8 TWiMODLORAWAN_McastData::AppPayload[WiMODLORAWAN_APP_PAYLOAD_LEN]

The application layer payload

## ◆ ChannelIndex

UINT8 TWiMODLORAWAN_McastData::ChannelIndex

used channel index (

See also
  TLoRaWAN_Channel_* definitions)

## ◆ DataRateIndex

UINT8 TWiMODLORAWAN_McastData::DataRateIndex

used data rate index (

See also
  TLoRaWANDataRate*)

## ◆ DeviceAddress

UINT32 TWiMODLORAWAN_McastData::DeviceAddress

address of the WiMOD within the Multicast context of LoRaWAN network

## ◆ LoRaWANPort

UINT8 TWiMODLORAWAN_McastData::LoRaWANPort

The port number on which the data has been received

## ◆ OptionalInfoAvaiable

bool TWiMODLORAWAN_McastData::OptionalInfoAvaiable

are the optional value fields available

## ◆ RSSI

INT8 TWiMODLORAWAN_McastData::RSSI

RSSI value for the received packet

## ◆ RxSlot

UINT8 TWiMODLORAWAN_McastData::RxSlot

number of the rx slot that contained the message

## ◆ SNR

INT8 TWiMODLORAWAN_McastData::SNR

SNR value for the received packet

## ◆ StatusFormat

UINT8 TWiMODLORAWAN_McastData::StatusFormat

Status/Format Field set by WiMOD;

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_ProLink_IDs.h