| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Typedefs | Enumerations
WiMOD_SAP_LORAWAN_IDs_IN865.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Typedefs
typedef enum TLoRaWANDataRateIN865 | TLoRaWANDataRateIN865
| LoRa data rate definitions for India 865 MHz Band. More...
typedef enum TLoRaWAN_Channel_India | TLoRaWAN_Channel_India
| Channel definition for India.
typedef enum TLoRaWAN_Channel_IndiaTwo | TLoRaWAN_Channel_IndiaTwo
| Channel definition for India.

## Enumerations
enum | TLoRaWANDataRateIN865 { LoRaWAN_DataRate_IN865_LoRa_SF12_125kHz = 0, LoRaWAN_DataRate_IN865_LoRa_SF11_125kHz, LoRaWAN_DataRate_IN865_LoRa_SF10_125kHz, LoRaWAN_DataRate_IN865_LoRa_SF9_125kHz, LoRaWAN_DataRate_IN865_LoRa_SF8_125kHz, LoRaWAN_DataRate_IN865_LoRa_SF7_125kHz, LoRaWAN_DataRate_IN865_LoRa_FSK = 7 }
| LoRa data rate definitions for India 865 MHz Band. More...
enum | TLoRaWAN_Channel_India { LoRaWAN_Channel_India_865_062_5_Mhz = 0, LoRaWAN_Channel_India_865_402_5_Mhz = 1, LoRaWAN_Channel_India_865_985_Mhz = 2, LoRaWAN_Channel_India_866_550_Mhz = 128 }
| Channel definition for India. More...
enum | TLoRaWAN_Channel_IndiaTwo { LoRaWAN_Channel_India2_865_062_5_Mhz = 0, LoRaWAN_Channel_India2_865_402_5_Mhz = 1, LoRaWAN_Channel_India2_865_985_Mhz = 2, LoRaWAN_Channel_India2_866_550_Mhz = 128 }
| Channel definition for India. More...

## Typedef Documentation

## ◆ TLoRaWANDataRateIN865

typedef enum TLoRaWANDataRateIN865 TLoRaWANDataRateIN865

LoRa data rate definitions for India 865 MHz Band.

Version
  0.1

## Enumeration Type Documentation

## ◆ TLoRaWAN_Channel_India

enum TLoRaWAN_Channel_India

Channel definition for India.

Enumerator
LoRaWAN_Channel_India_865_062_5_Mhz | carrier frequency of 865.062 500 MHz
LoRaWAN_Channel_India_865_402_5_Mhz | carrier frequency of 865.402 500 MHz
LoRaWAN_Channel_India_865_985_Mhz | carrier frequency of 865.985 MHz
LoRaWAN_Channel_India_866_550_Mhz | carrier frequency of 866.550 MHz

## ◆ TLoRaWAN_Channel_IndiaTwo

enum TLoRaWAN_Channel_IndiaTwo

Channel definition for India.

Enumerator
LoRaWAN_Channel_India2_865_062_5_Mhz | carrier frequency of 865.062 500 MHz
LoRaWAN_Channel_India2_865_402_5_Mhz | carrier frequency of 865.402 500 MHz
LoRaWAN_Channel_India2_865_985_Mhz | carrier frequency of 865.985 MHz
LoRaWAN_Channel_India2_866_550_Mhz | carrier frequency of 866.550 MHz

## ◆ TLoRaWANDataRateIN865

enum TLoRaWANDataRateIN865

LoRa data rate definitions for India 865 MHz Band.

Version
  0.1

Enumerator
LoRaWAN_DataRate_IN865_LoRa_SF12_125kHz | LoRa Spreading factor 12 using 125kHz bandwidth
LoRaWAN_DataRate_IN865_LoRa_SF11_125kHz | LoRa Spreading factor 11 using 125kHz bandwidth
LoRaWAN_DataRate_IN865_LoRa_SF10_125kHz | LoRa Spreading factor 10 using 125kHz bandwidth
LoRaWAN_DataRate_IN865_LoRa_SF9_125kHz | LoRa Spreading factor 9 using 125kHz bandwidth
LoRaWAN_DataRate_IN865_LoRa_SF8_125kHz | LoRa Spreading factor 8 using 125kHz bandwidth
LoRaWAN_DataRate_IN865_LoRa_SF7_125kHz | LoRa Spreading factor 7 using 125kHz bandwidth
LoRaWAN_DataRate_IN865_LoRa_FSK | FSK modulation; LoRa settings not applicable