| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

TWiMODLRHCI Member List

This is the complete list of members for TWiMODLRHCI, including all inherited members.

begin(void) | TWiMODLRHCI | virtual
EnableWakeupSequence(bool flag) (defined in TWiMODLRHCI) | TWiMODLRHCI |
end(void) | TWiMODLRHCI | virtual
GetRxMessage(void) (defined in TWiMODLRHCI) | TWiMODLRHCI |
PostMessage(UINT8 sapID, UINT8 msgID, UINT8 *payload, UINT16 length) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
Process(void) | TWiMODLRHCI |
ProcessRxMessage(UINT8 *rxBuffer, UINT16 length) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
RegisterStackErrorClient(TWiMODStackErrorClient cb) (defined in TWiMODLRHCI) | TWiMODLRHCI |
SendHCIMessage(UINT8 dstSapID, UINT8 msgID, UINT8 rxMsgID, UINT8 *payload, UINT16 length) | TWiMODLRHCI |
SendHCIMessageWithoutRx(UINT8 dstSapID, UINT8 msgID, UINT8 *payload, UINT16 length) | TWiMODLRHCI |
SendPacket(UINT8 *txData, UINT16 length) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
SendWakeUpSequence(void) | TWiMODLRHCI |
TComSlipClient() (defined in TComSlipClient) | TComSlipClient | inline
TWiMODLRHCI(Stream &s) | TWiMODLRHCI |
WaitForResponse(UINT8 rxSapID, UINT8 rxMsgID) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
~TComSlipClient() (defined in TComSlipClient) | TComSlipClient | inline virtual
~TWiMODLRHCI(void) | TWiMODLRHCI |