| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLR_RLT_Status Struct Reference

Structure containing a general RadioLink HCI message. More...

`#include <SAP/WiMOD_SAP_RLT_IDs.h>`

## Public Attributes
UINT8 | TestStatus
UINT16 | LocalTxCounter
UINT16 | LocalRxCounter
UINT16 | PeerTxCounter
UINT16 | PeerRxCounter
UINT16 | LocalRSSI
UINT16 | PeerRSSI
UINT8 | LocalSNR
UINT8 | PeerSNR

## Detailed Description

Structure containing a general RadioLink HCI message.

## Member Data Documentation

## ◆ LocalRSSI

UINT16 TWiMODLR_RLT_Status::LocalRSSI

RSSI value [dBm] of last received packet on local device

## ◆ LocalRxCounter

UINT16 TWiMODLR_RLT_Status::LocalRxCounter

Number of received packets on local device

## ◆ LocalSNR

UINT8 TWiMODLR_RLT_Status::LocalSNR

SNR value [dB] of last received packet on local device

## ◆ LocalTxCounter

UINT16 TWiMODLR_RLT_Status::LocalTxCounter

Number of transmitted packets from local device to peer device

## ◆ PeerRSSI

UINT16 TWiMODLR_RLT_Status::PeerRSSI

RSSI value [dBm] of last received packet on peer device

## ◆ PeerRxCounter

UINT16 TWiMODLR_RLT_Status::PeerRxCounter

Number of packets received on peer device

## ◆ PeerSNR

UINT8 TWiMODLR_RLT_Status::PeerSNR

SNR value [dB] of last received value on peer device

## ◆ PeerTxCounter

UINT16 TWiMODLR_RLT_Status::PeerTxCounter

Number of transmitted packets from peer device to local device

## ◆ TestStatus

UINT8 TWiMODLR_RLT_Status::TestStatus

Status of Test; 0 = OK, 1 = start of new test run

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_RLT_IDs.h