| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLR_SensorApp_Config Struct Reference

Structure containing a general RadioLink HCI message. More...

`#include <SAP/WiMOD_SAP_SensorApp_IDs.h>`

## Public Attributes
UINT8 | Status
TSensorApp_Mode | Mode
UINT8 | Options
UINT32 | SendingPeriod
UINT32 | LinkTimeout

## Detailed Description

Structure containing a general RadioLink HCI message.

## Member Data Documentation

## ◆ LinkTimeout

UINT32 TWiMODLR_SensorApp_Config::LinkTimeout

Rx Link Timeout in ms

## ◆ Mode

TSensorApp_Mode TWiMODLR_SensorApp_Config::Mode

Mode of operation

## ◆ Options

UINT8 TWiMODLR_SensorApp_Config::Options

(activated) Options;

See also
  SENSORAPP_OPTION_* defines

## ◆ SendingPeriod

UINT32 TWiMODLR_SensorApp_Config::SendingPeriod

Tx Sensor Data Period in ms

## ◆ Status

UINT8 TWiMODLR_SensorApp_Config::Status

Status/Format Field set by WiMOD; (WiMOD --> Host only)

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_SensorApp_IDs.h