| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLR_SensorApp_AckSensorData Struct Reference

Structure containing the data of an Ack of the SensorApp. More...

`#include <SAP/WiMOD_SAP_SensorApp_IDs.h>`

## Public Attributes
UINT8 | StatusFormat
UINT8 | DestGroupAddress
UINT16 | DestDevAddress
UINT8 | SourceGroupAddress
UINT16 | SourceDevAddress
UINT8 | DigitalInputs
INT16 | RSSI
INT8 | SNR
UINT32 | RxTime
bool | OptionalInfoAvaiable

## Detailed Description

Structure containing the data of an Ack of the SensorApp.

## Member Data Documentation

## ◆ DestDevAddress

UINT16 TWiMODLR_SensorApp_AckSensorData::DestDevAddress

destination device address

## ◆ DestGroupAddress

UINT8 TWiMODLR_SensorApp_AckSensorData::DestGroupAddress

destination group address

## ◆ DigitalInputs

UINT8 TWiMODLR_SensorApp_AckSensorData::DigitalInputs

Sensor Values;

See also
  SENSORAPP_DIGITAL_INPUT* defines

## ◆ OptionalInfoAvaiable

bool TWiMODLR_SensorApp_AckSensorData::OptionalInfoAvaiable

internal flag indicating of optional fields are present / valid

## ◆ RSSI

INT16 TWiMODLR_SensorApp_AckSensorData::RSSI

Received Signal Strength Indicator [dBm], signed integer

## ◆ RxTime

UINT32 TWiMODLR_SensorApp_AckSensorData::RxTime

timestamp from RTC

## ◆ SNR

INT8 TWiMODLR_SensorApp_AckSensorData::SNR

Signal to Noise Ratio [dB], signed integer

## ◆ SourceDevAddress

UINT16 TWiMODLR_SensorApp_AckSensorData::SourceDevAddress

device address of message sender

## ◆ SourceGroupAddress

UINT8 TWiMODLR_SensorApp_AckSensorData::SourceGroupAddress

group address of message sender

## ◆ StatusFormat

UINT8 TWiMODLR_SensorApp_AckSensorData::StatusFormat

Status/Format Field set by WiMOD; (WiMOD --> Host only)

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_SensorApp_IDs.h