| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Classes | Typedefs
WiMODLR_BASE.h File Reference
`#include "Arduino.h"`
`#include <string.h>`
`#include "utils/WMDefs.h"`
`#include "utils/ComSLIP.h"`
`#include "HCI/WiMODLRHCI.h"`
`#include "utils/FreqCalc_SX127x.h"`
`#include "SAP/WiMOD_SAP_DEVMGMT.h"`
`#include "SAP/WiMOD_SAP_RadioLink.h"`
`#include "SAP/WiMOD_SAP_Generic.h"`
`#include "SAP/WiMOD_SAP_HWTest.h"`
Include dependency graph for WiMODLR_BASE.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Classes
class | WiMODLRBASE
| Main class representing the interface to the WiMOD running the firmware WiMODLR-BASE. More...

## Typedefs
typedef void(* | TDataLinkRxUDataIndClient) (UINT8 *data, UINT16 length)
typedef void(* | TDataLinkSendUdataIndClient) (UINT8 status)

## Typedef Documentation

## ◆ TDataLinkRxUDataIndClient

typedef void(* TDataLinkRxUDataIndClient) (UINT8 *data, UINT16 length)

THIS IS AN EXAMPLE IMPLEMENTATION ACCORDING THE THE HCI SPEC: V1.10 FOR FIRMWARE: LR-BASE Type definition for callback function that handles a 'RX U-Data event' for the DataLink service

## ◆ TDataLinkSendUdataIndClient

typedef void(* TDataLinkSendUdataIndClient) (UINT8 status)

Type definition for callback function that handles a 'TX U-Data event' for the DataLink service