| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

WiMOD_SAP_DevMgmt_Lorawan Member List

This is the complete list of members for WiMOD_SAP_DevMgmt_Lorawan, including all inherited members.

ClearRtcAlarm(UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
DispatchDeviceMgmtMessage(TWiMODLR_HCIMessage &rxMsg) (defined in WiMOD_SAP_DevMgmt) | WiMOD_SAP_DevMgmt |
GetAesKey(UINT8 *key, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt_Lorawan | virtual
GetDeviceInfo(TWiMODLR_DevMgmt_DevInfo *info, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt_Lorawan | virtual
GetDeviceInfo(TWiMODLR_DevMgmt_DevInfoLoRaWan *info, UINT8 *statusRsp) (defined in WiMOD_SAP_DevMgmt_Lorawan) | WiMOD_SAP_DevMgmt_Lorawan | virtual
GetFirmwareInfo(TWiMODLR_DevMgmt_FwInfo *info, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
GetHCIConfig(TWiMODLR_DevMgmt_HciConfig *hciConfig, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
GetOperationMode(TWiMOD_OperationMode *opMode, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
GetRadioConfig(TWiMODLR_DevMgmt_RadioConfig *radioCfg, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt_Lorawan | virtual
GetRtc(UINT32 *rtcTime, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
GetRtcAlarm(TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
GetSystemStatus(TWiMODLR_DevMgmt_SystemStatus *info, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt_Lorawan | virtual
GetSystemStatus(TWiMODLR_DevMgmt_SystemStatusLorawan *info, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt_Lorawan | virtual
Ping(UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
RegisterPowerUpIndicationClient(TDevMgmtPowerUpCallback cb) | WiMOD_SAP_DevMgmt |
RegisterRtcAlarmIndicationClient(TDevMgmtRtcAlarmCallback cb) | WiMOD_SAP_DevMgmt |
Reset(UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
ResetRadioConfig(UINT8 *statusRsp) | WiMOD_SAP_DevMgmt_Lorawan | virtual
SetAesKey(const UINT8 *key, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt_Lorawan | virtual
SetHCIConfig(TWiMODLR_DevMgmt_HciConfig &hciConfig, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
SetOperationMode(const TWiMOD_OperationMode opMode, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
SetRadioConfig(const TWiMODLR_DevMgmt_RadioConfig *radioCfg, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt_Lorawan | virtual
SetRadioMode(const TRadioCfg_RadioMode radioMode, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt_Lorawan | virtual
SetRtc(const UINT32 rtcTime, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
SetRtcAlarm(const TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, UINT8 *statusRsp) | WiMOD_SAP_DevMgmt | virtual
unsupportedCmd(UINT8 *statusRsp) (defined in WiMOD_SAP_DevMgmt_Lorawan) | WiMOD_SAP_DevMgmt_Lorawan | protected virtual
WiMOD_SAP_DevMgmt(TWiMODLRHCI *hci, UINT8 *buffer, UINT16 bufferSize) | WiMOD_SAP_DevMgmt |
WiMOD_SAP_DevMgmt_Lorawan(TWiMODLRHCI *hci, UINT8 *buffer, UINT16 bufferSize) | WiMOD_SAP_DevMgmt_Lorawan |
~WiMOD_SAP_DevMgmt(void) | WiMOD_SAP_DevMgmt | virtual
~WiMOD_SAP_DevMgmt_Lorawan(void) | WiMOD_SAP_DevMgmt_Lorawan | virtual