| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLORAWAN_TxIndData Struct Reference

Activation data structure for LoRa network activation. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

Inheritance diagram for TWiMODLORAWAN_TxIndData:
[legend]

## Public Attributes
TWiMODLORAWAN_OptIndInfos | FieldAvailability
UINT8 | StatusFormat
UINT8 | ChannelIndex
UINT8 | DataRateIndex
UINT8 | NumTxPackets
UINT8 | PowerLevel
UINT32 | RfMsgAirtime

## Detailed Description

Activation data structure for LoRa network activation.

## Member Data Documentation

## ◆ ChannelIndex

UINT8 TWiMODLORAWAN_TxIndData::ChannelIndex

used channel index (

See also
  TLoRaWAN_Channel_* definitions)

## ◆ DataRateIndex

UINT8 TWiMODLORAWAN_TxIndData::DataRateIndex

used data rate index (

See also
  TLoRaWANDataRate*)

## ◆ FieldAvailability

TWiMODLORAWAN_OptIndInfos TWiMODLORAWAN_TxIndData::FieldAvailability

indicator flag for optional infos

## ◆ NumTxPackets

UINT8 TWiMODLORAWAN_TxIndData::NumTxPackets

number of TX packet (for current operation; can be used as retransmission counter)

## ◆ PowerLevel

UINT8 TWiMODLORAWAN_TxIndData::PowerLevel

transmit power in dBm

## ◆ RfMsgAirtime

UINT32 TWiMODLORAWAN_TxIndData::RfMsgAirtime

airtime in ms of packet transmission

## ◆ StatusFormat

UINT8 TWiMODLORAWAN_TxIndData::StatusFormat

Status/Format field of response packet from WiMOD

See also
  TLoRaWanTxDataIndStatusFormat

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h