| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

WiMOD_SAP_LORAWAN_IDs_US915.h
Go to the documentation of this file.
1 //------------------------------------------------------------------------------
31 //------------------------------------------------------------------------------
32
33
34 /*
35 * THIS IS AN EXAMPLE IMPLEMENTATION ACCORDING THE THE HCI SPEC: V1.22 for US915 (V0.2)
36 * FOR FIRMWARE: LoRaWAN_EndNode_Modem
37 *
38 * SEE FILE: WiMOD_LoRaWAN_EndNode_Modem_US915_HCI_Spec_V0_2.pdf
39 * for detailed information
40 *
41 * Reference: RP002-1.0.1 LoRaWAN Regional Parameters document (LoRa Alliance)
42 *
43 */
44
45
46 #ifndef ARDUINO_SAP_WIMOD_SAP_LORAWAN_IDS_US915_H_
47 #define ARDUINO_SAP_WIMOD_SAP_LORAWAN_IDS_US915_H_
48 //------------------------------------------------------------------------------
49 //
50 // Section Includes Files
51 //
52 //------------------------------------------------------------------------------
53
55
56 #define WIMOD_LORAWAN_US915
57
58
59
60 // LoRa Radio Band Index
61 #define LORAWAN_BAND_US_915 2
64 // LoRa Data Rate Index
65
66 #define LORAWAN_DATA_RATE_US915_LORA_SF10_125KHZ 0
67 #define LORAWAN_DATA_RATE_US915_LORA_SF9_125KHZ 1
68 #define LORAWAN_DATA_RATE_US915_LORA_SF8_125KHZ 2
69 #define LORAWAN_DATA_RATE_US915_LORA_SF7_125KHZ 3
70 #define LORAWAN_DATA_RATE_US915_LORA_SF8_500KHZ_1 4
71 #define LORAWAN_DATA_RATE_US915_LORA_SF12_500KHZ 8
72 #define LORAWAN_DATA_RATE_US915_LORA_SF11_500KHZ 9
73 #define LORAWAN_DATA_RATE_US915_LORA_SF10_500KHZ 10
74 #define LORAWAN_DATA_RATE_US915_LORA_SF9_500KHZ 11
75 #define LORAWAN_DATA_RATE_US915_LORA_SF8_500KHZ_2 12
76 #define LORAWAN_DATA_RATE_US915_LORA_SF7_500KHZ 13
78 #define LORAWAN_DATA_RATE_US915_DR0 LORAWAN_DATA_RATE_US915_LORA_SF10_125KHZ
79 #define LORAWAN_DATA_RATE_US915_DR1 LORAWAN_DATA_RATE_US915_LORA_SF9_125KHZ
80 #define LORAWAN_DATA_RATE_US915_DR2 LORAWAN_DATA_RATE_US915_LORA_SF8_125KHZ
81 #define LORAWAN_DATA_RATE_US915_DR3 LORAWAN_DATA_RATE_US915_LORA_SF7_125KHZ
82 #define LORAWAN_DATA_RATE_US915_DR4 LORAWAN_DATA_RATE_US915_LORA_SF8_500KHZ_1
83 #define LORAWAN_DATA_RATE_US915_DR8 LORAWAN_DATA_RATE_US915_LORA_SF12_500KHZ
84 #define LORAWAN_DATA_RATE_US915_DR9 LORAWAN_DATA_RATE_US915_LORA_SF11_500KHZ
85 #define LORAWAN_DATA_RATE_US915_DR10 LORAWAN_DATA_RATE_US915_LORA_SF10_500KHZ
86 #define LORAWAN_DATA_RATE_US915_DR11 LORAWAN_DATA_RATE_US915_LORA_SF9_500KHZ
87 #define LORAWAN_DATA_RATE_US915_DR12 LORAWAN_DATA_RATE_US915_LORA_SF8_500KHZ_2
88 #define LORAWAN_DATA_RATE_US915_DR13 LORAWAN_DATA_RATE_US915_LORA_SF7_500KHZ
89
90
91
92 #define IS_LORAWAN_US915_DATA_RATE(x) ( ((x) == LORAWAN_DATA_RATE_US915_LORA_SF10_125KHZ ) || \
93 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF9_125KHZ ) || \
94 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF8_125KHZ ) || \
95 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF7_125KHZ ) || \
96 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF8_500KHZ_1) || \
97 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF12_500KHZ ) || \
98 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF11_500KHZ ) || \
99 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF10_500KHZ ) || \
100 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF9_500KHZ ) || \
101 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF8_500KHZ_2) || \
102 ((x) == LORAWAN_DATA_RATE_US915_LORA_SF7_500KHZ ) );
103
105
109 typedef enum TLoRaWANDataRateUS915
110 {
111 LoRaWAN_DataRate_US915_LoRa_SF10_125KHZ = 0,
112 LoRaWAN_DataRate_US915_LoRa_SF9_125KHZ = 1,
113 LoRaWAN_DataRate_US915_LoRa_SF8_125KHZ = 2,
114 LoRaWAN_DataRate_US915_LoRa_SF7_125KHZ = 3,
115 LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_1= 4,
116 LoRaWAN_DataRate_US915_LoRa_SF12_500KHZ = 8,
117 LoRaWAN_DataRate_US915_LoRa_SF11_500KHZ = 9,
118 LoRaWAN_DataRate_US915_LoRa_SF10_500KHZ = 10,
119 LoRaWAN_DataRate_US915_LoRa_SF9_500KHZ = 11,
120 LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_2= 12,
121 LoRaWAN_DataRate_US915_LoRa_SF7_500KHZ = 13,
122 } TLoRaWANDataRateUS915;
123
124
125
127
128 // LoRa Channel Index ( US915 )
129
130 // uplink
131 #define LORAWAN_CH_US_UP_902_3_MHZ 0
132 #define LORAWAN_CH_US_UP_902_5_MHZ 1
133 #define LORAWAN_CH_US_UP_902_7_MHZ 2
134 #define LORAWAN_CH_US_UP_902_9_MHZ 3
135 #define LORAWAN_CH_US_UP_903_1_MHZ 4
136 #define LORAWAN_CH_US_UP_903_3_MHZ 5
137 #define LORAWAN_CH_US_UP_903_5_MHZ 6
138 #define LORAWAN_CH_US_UP_903_7_MHZ 7
140 #define LORAWAN_CH_US_UP_903_9_MHZ 8
141 #define LORAWAN_CH_US_UP_904_1_MHZ 9
142 #define LORAWAN_CH_US_UP_904_3_MHZ 10
143 #define LORAWAN_CH_US_UP_904_5_MHZ 11
144 #define LORAWAN_CH_US_UP_904_7_MHZ 12
145 #define LORAWAN_CH_US_UP_904_9_MHZ 13
146 #define LORAWAN_CH_US_UP_905_1_MHZ 14
147 #define LORAWAN_CH_US_UP_905_3_MHZ 15
149 #define LORAWAN_CH_US_UP_905_5_MHZ 16
150 #define LORAWAN_CH_US_UP_905_7_MHZ 17
151 #define LORAWAN_CH_US_UP_905_9_MHZ 18
152 #define LORAWAN_CH_US_UP_906_1_MHZ 19
153 #define LORAWAN_CH_US_UP_906_3_MHZ 20
154 #define LORAWAN_CH_US_UP_906_5_MHZ 21
155 #define LORAWAN_CH_US_UP_906_7_MHZ 22
156 #define LORAWAN_CH_US_UP_906_9_MHZ 23
158 #define LORAWAN_CH_US_UP_907_1_MHZ 24
159 #define LORAWAN_CH_US_UP_907_3_MHZ 25
160 #define LORAWAN_CH_US_UP_907_5_MHZ 26
161 #define LORAWAN_CH_US_UP_907_7_MHZ 27
162 #define LORAWAN_CH_US_UP_907_9_MHZ 28
163 #define LORAWAN_CH_US_UP_908_1_MHZ 29
164 #define LORAWAN_CH_US_UP_908_3_MHZ 30
165 #define LORAWAN_CH_US_UP_908_5_MHZ 31
167 #define LORAWAN_CH_US_UP_908_7_MHZ 32
168 #define LORAWAN_CH_US_UP_908_9_MHZ 33
169 #define LORAWAN_CH_US_UP_909_1_MHZ 34
170 #define LORAWAN_CH_US_UP_909_3_MHZ 35
171 #define LORAWAN_CH_US_UP_909_5_MHZ 36
172 #define LORAWAN_CH_US_UP_909_7_MHZ 37
173 #define LORAWAN_CH_US_UP_909_9_MHZ 38
174 #define LORAWAN_CH_US_UP_910_1_MHZ 39
176 #define LORAWAN_CH_US_UP_910_3_MHZ 40
177 #define LORAWAN_CH_US_UP_910_5_MHZ 41
178 #define LORAWAN_CH_US_UP_910_7_MHZ 42
179 #define LORAWAN_CH_US_UP_910_9_MHZ 43
180 #define LORAWAN_CH_US_UP_911_1_MHZ 44
181 #define LORAWAN_CH_US_UP_911_3_MHZ 45
182 #define LORAWAN_CH_US_UP_911_5_MHZ 46
183 #define LORAWAN_CH_US_UP_911_7_MHZ 47
185 #define LORAWAN_CH_US_UP_911_9_MHZ 48
186 #define LORAWAN_CH_US_UP_912_1_MHZ 49
187 #define LORAWAN_CH_US_UP_912_3_MHZ 50
188 #define LORAWAN_CH_US_UP_912_5_MHZ 51
189 #define LORAWAN_CH_US_UP_912_7_MHZ 52
190 #define LORAWAN_CH_US_UP_912_9_MHZ 53
191 #define LORAWAN_CH_US_UP_913_1_MHZ 54
192 #define LORAWAN_CH_US_UP_913_3_MHZ 55
194 #define LORAWAN_CH_US_UP_913_5_MHZ 56
195 #define LORAWAN_CH_US_UP_913_7_MHZ 57
196 #define LORAWAN_CH_US_UP_913_9_MHZ 58
197 #define LORAWAN_CH_US_UP_914_1_MHZ 59
198 #define LORAWAN_CH_US_UP_914_3_MHZ 60
199 #define LORAWAN_CH_US_UP_914_5_MHZ 61
200 #define LORAWAN_CH_US_UP_914_7_MHZ 62
201 #define LORAWAN_CH_US_UP_914_9_MHZ 63
203 #define LORAWAN_CH_US_UP_903_0_MHZ 64
204 #define LORAWAN_CH_US_UP_904_6_MHZ 65
205 #define LORAWAN_CH_US_UP_906_2_MHZ 66
206 #define LORAWAN_CH_US_UP_907_8_MHZ 67
207 #define LORAWAN_CH_US_UP_909_4_MHZ 68
208 #define LORAWAN_CH_US_UP_911_0_MHZ 69
209 #define LORAWAN_CH_US_UP_912_6_MHZ 70
210 #define LORAWAN_CH_US_UP_914_2_MHZ 71
213 //downlink
214 #define LORAWAN_CH_US_DN_923_3_MHZ 0
215 #define LORAWAN_CH_US_DN_923_9_MHZ 1
216 #define LORAWAN_CH_US_DN_924_5_MHZ 2
217 #define LORAWAN_CH_US_DN_925_1_MHZ 3
218 #define LORAWAN_CH_US_DN_925_7_MHZ 4
219 #define LORAWAN_CH_US_DN_926_3_MHZ 5
220 #define LORAWAN_CH_US_DN_926_9_MHZ 6
221 #define LORAWAN_CH_US_DN_927_5_MHZ 7
222
223 #define LORAWAN_CH_US_DN_923_3_MHZ_2 8
224 #define LORAWAN_CH_US_DN_923_9_MHZ_2 9
225 #define LORAWAN_CH_US_DN_924_5_MHZ_2 10
226 #define LORAWAN_CH_US_DN_925_1_MHZ_2 11
227 #define LORAWAN_CH_US_DN_925_7_MHZ_2 12
228 #define LORAWAN_CH_US_DN_926_3_MHZ_2 13
229 #define LORAWAN_CH_US_DN_926_9_MHZ_2 14
230 #define LORAWAN_CH_US_DN_927_5_MHZ_2 15
231
232 #define LORAWAN_CH_US_DN_923_3_MHZ_3 16
233 #define LORAWAN_CH_US_DN_923_9_MHZ_3 17
234 #define LORAWAN_CH_US_DN_924_5_MHZ_3 18
235 #define LORAWAN_CH_US_DN_925_1_MHZ_3 19
236 #define LORAWAN_CH_US_DN_925_7_MHZ_3 20
237 #define LORAWAN_CH_US_DN_926_3_MHZ_3 21
238 #define LORAWAN_CH_US_DN_926_9_MHZ_3 22
239 #define LORAWAN_CH_US_DN_927_5_MHZ_3 23
240
241 #define LORAWAN_CH_US_DN_923_3_MHZ_4 24
242 #define LORAWAN_CH_US_DN_923_9_MHZ_4 25
243 #define LORAWAN_CH_US_DN_924_5_MHZ_4 26
244 #define LORAWAN_CH_US_DN_925_1_MHZ_4 27
245 #define LORAWAN_CH_US_DN_925_7_MHZ_4 28
246 #define LORAWAN_CH_US_DN_926_3_MHZ_4 29
247 #define LORAWAN_CH_US_DN_926_9_MHZ_4 30
248 #define LORAWAN_CH_US_DN_927_5_MHZ_4 31
249
250 #define LORAWAN_CH_US_DN_923_3_MHZ_5 32
251 #define LORAWAN_CH_US_DN_923_9_MHZ_5 33
252 #define LORAWAN_CH_US_DN_924_5_MHZ_5 34
253 #define LORAWAN_CH_US_DN_925_1_MHZ_5 35
254 #define LORAWAN_CH_US_DN_925_7_MHZ_5 36
255 #define LORAWAN_CH_US_DN_926_3_MHZ_5 37
256 #define LORAWAN_CH_US_DN_926_9_MHZ_5 38
257 #define LORAWAN_CH_US_DN_927_5_MHZ_5 39
258
259 #define LORAWAN_CH_US_DN_923_3_MHZ_6 40
260 #define LORAWAN_CH_US_DN_923_9_MHZ_6 41
261 #define LORAWAN_CH_US_DN_924_5_MHZ_6 42
262 #define LORAWAN_CH_US_DN_925_1_MHZ_6 43
263 #define LORAWAN_CH_US_DN_925_7_MHZ_6 44
264 #define LORAWAN_CH_US_DN_926_3_MHZ_6 45
265 #define LORAWAN_CH_US_DN_926_9_MHZ_6 46
266 #define LORAWAN_CH_US_DN_927_5_MHZ_6 47
267
268 #define LORAWAN_CH_US_DN_923_3_MHZ_7 48
269 #define LORAWAN_CH_US_DN_923_9_MHZ_7 49
270 #define LORAWAN_CH_US_DN_924_5_MHZ_7 50
271 #define LORAWAN_CH_US_DN_925_1_MHZ_7 51
272 #define LORAWAN_CH_US_DN_925_7_MHZ_7 52
273 #define LORAWAN_CH_US_DN_926_3_MHZ_7 53
274 #define LORAWAN_CH_US_DN_926_9_MHZ_7 54
275 #define LORAWAN_CH_US_DN_927_5_MHZ_7 55
276
277 #define LORAWAN_CH_US_DN_923_3_MHZ_8 56
278 #define LORAWAN_CH_US_DN_923_9_MHZ_8 57
279 #define LORAWAN_CH_US_DN_924_5_MHZ_8 58
280 #define LORAWAN_CH_US_DN_925_1_MHZ_8 59
281 #define LORAWAN_CH_US_DN_925_7_MHZ_8 60
282 #define LORAWAN_CH_US_DN_926_3_MHZ_8 61
283 #define LORAWAN_CH_US_DN_926_9_MHZ_8 62
284 #define LORAWAN_CH_US_DN_927_5_MHZ_8 63
285
286 #define LORAWAN_CH_US_DN_923_3_MHZ_9 64
287 #define LORAWAN_CH_US_DN_923_9_MHZ_9 65
288 #define LORAWAN_CH_US_DN_924_5_MHZ_9 66
289 #define LORAWAN_CH_US_DN_925_1_MHZ_9 67
290 #define LORAWAN_CH_US_DN_925_7_MHZ_9 68
291 #define LORAWAN_CH_US_DN_926_3_MHZ_9 69
292 #define LORAWAN_CH_US_DN_926_9_MHZ_9 70
293 #define LORAWAN_CH_US_DN_927_5_MHZ_9 71
294
295 #define LORAWAN_CH_US_DN_923_3_MHZ_10 128
296
297
298 #define IS_LORAWAN_CH_US915_UP(x) ( ((x) >= LORAWAN_CH_US_UP_902_3_MHZ) && \
299 ((x) <= LORAWAN_CH_US_UP_914_2_MHZ) )
300
301
302 #define IS_LORAWAN_CH_US915_DN(x) ( (((x) >= LORAWAN_CH_US_DN_923_3_MHZ) && \
303 ((x) <= LORAWAN_CH_US_DN_927_5_MHZ_9) ) || \
304 ((x) == LORAWAN_CH_US_DN_923_3_MHZ_10) )
305
306
308
312 typedef enum TLoRaWAN_Channel_US_UP
313 {
314 LoRaWAN_Channel_US_UP_902_3_MHZ = 0,
315 LoRaWAN_Channel_US_UP_902_5_MHZ = 1,
316 LoRaWAN_Channel_US_UP_902_7_MHZ = 2,
317 LoRaWAN_Channel_US_UP_902_9_MHZ = 3,
318 LoRaWAN_Channel_US_UP_903_1_MHZ = 4,
319 LoRaWAN_Channel_US_UP_903_3_MHZ = 5,
320 LoRaWAN_Channel_US_UP_903_5_MHZ = 6,
321 LoRaWAN_Channel_US_UP_903_7_MHZ = 7,
323 LoRaWAN_Channel_US_UP_903_9_MHZ = 8,
324 LoRaWAN_Channel_US_UP_904_1_MHZ = 9,
325 LoRaWAN_Channel_US_UP_904_3_MHZ = 10,
326 LoRaWAN_Channel_US_UP_904_5_MHZ = 11,
327 LoRaWAN_Channel_US_UP_904_7_MHZ = 12,
328 LoRaWAN_Channel_US_UP_904_9_MHZ = 13,
329 LoRaWAN_Channel_US_UP_905_1_MHZ = 14,
330 LoRaWAN_Channel_US_UP_905_3_MHZ = 15,
332 LoRaWAN_Channel_US_UP_905_5_MHZ = 16,
333 LoRaWAN_Channel_US_UP_905_7_MHZ = 17,
334 LoRaWAN_Channel_US_UP_905_9_MHZ = 18,
335 LoRaWAN_Channel_US_UP_906_1_MHZ = 19,
336 LoRaWAN_Channel_US_UP_906_3_MHZ = 20,
337 LoRaWAN_Channel_US_UP_906_5_MHZ = 21,
338 LoRaWAN_Channel_US_UP_906_7_MHZ = 22,
339 LoRaWAN_Channel_US_UP_906_9_MHZ = 23,
341 LoRaWAN_Channel_US_UP_907_1_MHZ = 24,
342 LoRaWAN_Channel_US_UP_907_3_MHZ = 25,
343 LoRaWAN_Channel_US_UP_907_5_MHZ = 26,
344 LoRaWAN_Channel_US_UP_907_7_MHZ = 27,
345 LoRaWAN_Channel_US_UP_907_9_MHZ = 28,
346 LoRaWAN_Channel_US_UP_908_1_MHZ = 29,
347 LoRaWAN_Channel_US_UP_908_3_MHZ = 30,
348 LoRaWAN_Channel_US_UP_908_5_MHZ = 31,
350 LoRaWAN_Channel_US_UP_908_7_MHZ = 32,
351 LoRaWAN_Channel_US_UP_908_9_MHZ = 33,
352 LoRaWAN_Channel_US_UP_909_1_MHZ = 34,
353 LoRaWAN_Channel_US_UP_909_3_MHZ = 35,
354 LoRaWAN_Channel_US_UP_909_5_MHZ = 36,
355 LoRaWAN_Channel_US_UP_909_7_MHZ = 37,
356 LoRaWAN_Channel_US_UP_909_9_MHZ = 38,
357 LoRaWAN_Channel_US_UP_910_1_MHZ = 39,
359 LoRaWAN_Channel_US_UP_910_3_MHZ = 40,
360 LoRaWAN_Channel_US_UP_910_5_MHZ = 41,
361 LoRaWAN_Channel_US_UP_910_7_MHZ = 42,
362 LoRaWAN_Channel_US_UP_910_9_MHZ = 43,
363 LoRaWAN_Channel_US_UP_911_1_MHZ = 44,
364 LoRaWAN_Channel_US_UP_911_3_MHZ = 45,
365 LoRaWAN_Channel_US_UP_911_5_MHZ = 46,
366 LoRaWAN_Channel_US_UP_911_7_MHZ = 47,
368 LoRaWAN_Channel_US_UP_911_9_MHZ = 48,
369 LoRaWAN_Channel_US_UP_912_1_MHZ = 49,
370 LoRaWAN_Channel_US_UP_912_3_MHZ = 50,
371 LoRaWAN_Channel_US_UP_912_5_MHZ = 51,
372 LoRaWAN_Channel_US_UP_912_7_MHZ = 52,
373 LoRaWAN_Channel_US_UP_912_9_MHZ = 53,
374 LoRaWAN_Channel_US_UP_913_1_MHZ = 54,
375 LoRaWAN_Channel_US_UP_913_3_MHZ = 55,
377 LoRaWAN_Channel_US_UP_913_5_MHZ = 56,
378 LoRaWAN_Channel_US_UP_913_7_MHZ = 57,
379 LoRaWAN_Channel_US_UP_913_9_MHZ = 58,
380 LoRaWAN_Channel_US_UP_914_1_MHZ = 59,
381 LoRaWAN_Channel_US_UP_914_3_MHZ = 60,
382 LoRaWAN_Channel_US_UP_914_5_MHZ = 61,
383 LoRaWAN_Channel_US_UP_914_7_MHZ = 62,
384 LoRaWAN_Channel_US_UP_914_9_MHZ = 63,
386 LoRaWAN_Channel_US_UP_903_0_MHZ = 64,
387 LoRaWAN_Channel_US_UP_904_6_MHZ = 65,
388 LoRaWAN_Channel_US_UP_906_2_MHZ = 66,
389 LoRaWAN_Channel_US_UP_907_8_MHZ = 67,
390 LoRaWAN_Channel_US_UP_909_4_MHZ = 68,
391 LoRaWAN_Channel_US_UP_911_0_MHZ = 69,
392 LoRaWAN_Channel_US_UP_912_6_MHZ = 70,
393 LoRaWAN_Channel_US_UP_914_2_MHZ = 71,
394 } TLoRaWAN_Channel_US_UP;
395
399 typedef enum TLoRaWAN_Channel_US_DN
400 {
401 LoRaWAN_Channel_US_DN_923_3_MHz = 0,
402 LoRaWAN_Channel_US_DN_923_9_MHz = 1,
403 LoRaWAN_Channel_US_DN_924_5_MHz = 2,
404 LoRaWAN_Channel_US_DN_925_1_MHz = 3,
405 LoRaWAN_Channel_US_DN_925_7_MHz = 4,
406 LoRaWAN_Channel_US_DN_926_3_MHz = 5,
407 LoRaWAN_Channel_US_DN_926_9_MHz = 6,
408 LoRaWAN_Channel_US_DN_927_5_MHz = 7,
410 LoRaWAN_Channel_US_DN_923_3_MHz_2 = 8,
411 LoRaWAN_Channel_US_DN_923_9_MHz_2 = 9,
412 LoRaWAN_Channel_US_DN_924_5_MHz_2 = 10,
413 LoRaWAN_Channel_US_DN_925_1_MHz_2 = 11,
414 LoRaWAN_Channel_US_DN_925_7_MHz_2 = 12,
415 LoRaWAN_Channel_US_DN_926_3_MHz_2 = 13,
416 LoRaWAN_Channel_US_DN_926_9_MHz_2 = 14,
417 LoRaWAN_Channel_US_DN_927_5_MHz_2 = 15,
419 LoRaWAN_Channel_US_DN_923_3_MHz_3 = 16,
420 LoRaWAN_Channel_US_DN_923_9_MHz_3 = 17,
421 LoRaWAN_Channel_US_DN_924_5_MHz_3 = 18,
422 LoRaWAN_Channel_US_DN_925_1_MHz_3 = 19,
423 LoRaWAN_Channel_US_DN_925_7_MHz_3 = 20,
424 LoRaWAN_Channel_US_DN_926_3_MHz_3 = 21,
425 LoRaWAN_Channel_US_DN_926_9_MHz_3 = 22,
426 LoRaWAN_Channel_US_DN_927_5_MHz_3 = 23,
428 LoRaWAN_Channel_US_DN_923_3_MHz_4 = 24,
429 LoRaWAN_Channel_US_DN_923_9_MHz_4 = 25,
430 LoRaWAN_Channel_US_DN_924_5_MHz_4 = 26,
431 LoRaWAN_Channel_US_DN_925_1_MHz_4 = 27,
432 LoRaWAN_Channel_US_DN_925_7_MHz_4 = 28,
433 LoRaWAN_Channel_US_DN_926_3_MHz_4 = 29,
434 LoRaWAN_Channel_US_DN_926_9_MHz_4 = 30,
435 LoRaWAN_Channel_US_DN_927_5_MHz_4 = 31,
437 LoRaWAN_Channel_US_DN_923_3_MHz_5 = 32,
438 LoRaWAN_Channel_US_DN_923_9_MHz_5 = 33,
439 LoRaWAN_Channel_US_DN_924_5_MHz_5 = 34,
440 LoRaWAN_Channel_US_DN_925_1_MHz_5 = 35,
441 LoRaWAN_Channel_US_DN_925_7_MHz_5 = 36,
442 LoRaWAN_Channel_US_DN_926_3_MHz_5 = 37,
443 LoRaWAN_Channel_US_DN_926_9_MHz_5 = 38,
444 LoRaWAN_Channel_US_DN_927_5_MHz_5 = 39,
446 LoRaWAN_Channel_US_DN_923_3_MHz_6 = 40,
447 LoRaWAN_Channel_US_DN_923_9_MHz_6 = 41,
448 LoRaWAN_Channel_US_DN_924_5_MHz_6 = 42,
449 LoRaWAN_Channel_US_DN_925_1_MHz_6 = 43,
450 LoRaWAN_Channel_US_DN_925_7_MHz_6 = 44,
451 LoRaWAN_Channel_US_DN_926_3_MHz_6 = 45,
452 LoRaWAN_Channel_US_DN_926_9_MHz_6 = 46,
453 LoRaWAN_Channel_US_DN_927_5_MHz_6 = 47,
455 LoRaWAN_Channel_US_DN_923_3_MHz_7 = 48,
456 LoRaWAN_Channel_US_DN_923_9_MHz_7 = 49,
457 LoRaWAN_Channel_US_DN_924_5_MHz_7 = 50,
458 LoRaWAN_Channel_US_DN_925_1_MHz_7 = 51,
459 LoRaWAN_Channel_US_DN_925_7_MHz_7 = 52,
460 LoRaWAN_Channel_US_DN_926_3_MHz_7 = 53,
461 LoRaWAN_Channel_US_DN_926_9_MHz_7 = 54,
462 LoRaWAN_Channel_US_DN_927_5_MHz_7 = 55,
464 LoRaWAN_Channel_US_DN_923_3_MHz_8 = 56,
465 LoRaWAN_Channel_US_DN_923_9_MHz_8 = 57,
466 LoRaWAN_Channel_US_DN_924_5_MHz_8 = 58,
467 LoRaWAN_Channel_US_DN_925_1_MHz_8 = 59,
468 LoRaWAN_Channel_US_DN_925_7_MHz_8 = 60,
469 LoRaWAN_Channel_US_DN_926_3_MHz_8 = 61,
470 LoRaWAN_Channel_US_DN_926_9_MHz_8 = 62,
471 LoRaWAN_Channel_US_DN_927_5_MHz_8 = 63,
473 LoRaWAN_Channel_US_DN_923_3_MHz_9 = 64,
474 LoRaWAN_Channel_US_DN_923_9_MHz_9 = 65,
475 LoRaWAN_Channel_US_DN_924_5_MHz_9 = 66,
476 LoRaWAN_Channel_US_DN_925_1_MHz_9 = 67,
477 LoRaWAN_Channel_US_DN_925_7_MHz_9 = 68,
478 LoRaWAN_Channel_US_DN_926_3_MHz_9 = 69,
479 LoRaWAN_Channel_US_DN_926_9_MHz_9 = 70,
480 LoRaWAN_Channel_US_DN_927_5_MHz_9 = 71,
482 LoRaWAN_Channel_US_DN_923_3_MHz_10 = 128,
483 } TLoRaWAN_Channel_US_DN;
484
485
486 #endif /* ARDUINO_SAP_WIMOD_SAP_LORAWAN_IDS_US915_H_ */
LoRaWAN_Channel_US_DN_926_3_MHz_8
@ LoRaWAN_Channel_US_DN_926_3_MHz_8
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:469
LoRaWAN_Channel_US_UP_911_1_MHZ
@ LoRaWAN_Channel_US_UP_911_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:363
LoRaWAN_Channel_US_DN_926_9_MHz_3
@ LoRaWAN_Channel_US_DN_926_9_MHz_3
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:425
LoRaWAN_Channel_US_DN_923_9_MHz_9
@ LoRaWAN_Channel_US_DN_923_9_MHz_9
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:474
LoRaWAN_Channel_US_DN_925_1_MHz_5
@ LoRaWAN_Channel_US_DN_925_1_MHz_5
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:440
LoRaWAN_Channel_US_DN_925_7_MHz
@ LoRaWAN_Channel_US_DN_925_7_MHz
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:405
LoRaWAN_Channel_US_UP_912_1_MHZ
@ LoRaWAN_Channel_US_UP_912_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:369
LoRaWAN_Channel_US_DN_923_3_MHz_6
@ LoRaWAN_Channel_US_DN_923_3_MHz_6
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:446
LoRaWAN_Channel_US_UP_912_9_MHZ
@ LoRaWAN_Channel_US_UP_912_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:373
LoRaWAN_Channel_US_UP_904_5_MHZ
@ LoRaWAN_Channel_US_UP_904_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:326
LoRaWAN_Channel_US_UP_911_3_MHZ
@ LoRaWAN_Channel_US_UP_911_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:364
LoRaWAN_Channel_US_UP_909_1_MHZ
@ LoRaWAN_Channel_US_UP_909_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:352
LoRaWAN_Channel_US_DN_923_3_MHz_2
@ LoRaWAN_Channel_US_DN_923_3_MHz_2
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:410
LoRaWAN_Channel_US_UP_910_3_MHZ
@ LoRaWAN_Channel_US_UP_910_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:359
LoRaWAN_Channel_US_DN_926_3_MHz_4
@ LoRaWAN_Channel_US_DN_926_3_MHz_4
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:433
TLoRaWANDataRateUS915
TLoRaWANDataRateUS915
LoRa data rate definitions for US 915 MHz Band.
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:109
LoRaWAN_Channel_US_DN_924_5_MHz_6
@ LoRaWAN_Channel_US_DN_924_5_MHz_6
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:448
LoRaWAN_Channel_US_UP_908_3_MHZ
@ LoRaWAN_Channel_US_UP_908_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:347
LoRaWAN_Channel_US_UP_913_3_MHZ
@ LoRaWAN_Channel_US_UP_913_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:375
LoRaWAN_Channel_US_UP_908_1_MHZ
@ LoRaWAN_Channel_US_UP_908_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:346
LoRaWAN_Channel_US_UP_902_7_MHZ
@ LoRaWAN_Channel_US_UP_902_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:316
LoRaWAN_Channel_US_UP_911_0_MHZ
@ LoRaWAN_Channel_US_UP_911_0_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:391
LoRaWAN_Channel_US_UP_910_9_MHZ
@ LoRaWAN_Channel_US_UP_910_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:362
LoRaWAN_Channel_US_DN_925_1_MHz_2
@ LoRaWAN_Channel_US_DN_925_1_MHz_2
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:413
LoRaWAN_Channel_US_DN_925_7_MHz_2
@ LoRaWAN_Channel_US_DN_925_7_MHz_2
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:414
LoRaWAN_Channel_US_DN_924_5_MHz_4
@ LoRaWAN_Channel_US_DN_924_5_MHz_4
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:430
LoRaWAN_Channel_US_UP_904_7_MHZ
@ LoRaWAN_Channel_US_UP_904_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:327
LoRaWAN_Channel_US_UP_909_9_MHZ
@ LoRaWAN_Channel_US_UP_909_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:356
LoRaWAN_Channel_US_DN_925_7_MHz_4
@ LoRaWAN_Channel_US_DN_925_7_MHz_4
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:432
LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_1
@ LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_1
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:115
LoRaWAN_Channel_US_UP_903_3_MHZ
@ LoRaWAN_Channel_US_UP_903_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:319
LoRaWAN_Channel_US_DN_926_9_MHz_7
@ LoRaWAN_Channel_US_DN_926_9_MHz_7
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:461
LoRaWAN_Channel_US_DN_926_9_MHz_2
@ LoRaWAN_Channel_US_DN_926_9_MHz_2
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:416
LoRaWAN_Channel_US_UP_910_7_MHZ
@ LoRaWAN_Channel_US_UP_910_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:361
LoRaWAN_Channel_US_DN_927_5_MHz_2
@ LoRaWAN_Channel_US_DN_927_5_MHz_2
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:417
LoRaWAN_Channel_US_UP_914_9_MHZ
@ LoRaWAN_Channel_US_UP_914_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:384
LoRaWAN_Channel_US_UP_908_9_MHZ
@ LoRaWAN_Channel_US_UP_908_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:351
LoRaWAN_DataRate_US915_LoRa_SF10_500KHZ
@ LoRaWAN_DataRate_US915_LoRa_SF10_500KHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:118
LoRaWAN_Channel_US_DN_924_5_MHz_5
@ LoRaWAN_Channel_US_DN_924_5_MHz_5
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:439
LoRaWAN_Channel_US_UP_907_7_MHZ
@ LoRaWAN_Channel_US_UP_907_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:344
LoRaWAN_Channel_US_DN_923_9_MHz_8
@ LoRaWAN_Channel_US_DN_923_9_MHz_8
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:465
LoRaWAN_Channel_US_UP_914_5_MHZ
@ LoRaWAN_Channel_US_UP_914_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:382
LoRaWAN_Channel_US_DN_925_1_MHz_7
@ LoRaWAN_Channel_US_DN_925_1_MHz_7
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:458
LoRaWAN_Channel_US_UP_905_7_MHZ
@ LoRaWAN_Channel_US_UP_905_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:333
LoRaWAN_Channel_US_UP_909_7_MHZ
@ LoRaWAN_Channel_US_UP_909_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:355
LoRaWAN_Channel_US_UP_912_6_MHZ
@ LoRaWAN_Channel_US_UP_912_6_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:392
LoRaWAN_Channel_US_DN_923_3_MHz_8
@ LoRaWAN_Channel_US_DN_923_3_MHz_8
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:464
LoRaWAN_Channel_US_UP_907_9_MHZ
@ LoRaWAN_Channel_US_UP_907_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:345
LoRaWAN_Channel_US_DN_926_9_MHz_8
@ LoRaWAN_Channel_US_DN_926_9_MHz_8
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:470
LoRaWAN_Channel_US_DN_926_9_MHz_4
@ LoRaWAN_Channel_US_DN_926_9_MHz_4
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:434
LoRaWAN_Channel_US_UP_906_1_MHZ
@ LoRaWAN_Channel_US_UP_906_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:335
LoRaWAN_Channel_US_UP_902_9_MHZ
@ LoRaWAN_Channel_US_UP_902_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:317
LoRaWAN_Channel_US_DN_926_3_MHz_7
@ LoRaWAN_Channel_US_DN_926_3_MHz_7
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:460
LoRaWAN_Channel_US_UP_906_9_MHZ
@ LoRaWAN_Channel_US_UP_906_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:339
LoRaWAN_DataRate_US915_LoRa_SF11_500KHZ
@ LoRaWAN_DataRate_US915_LoRa_SF11_500KHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:117
LoRaWAN_DataRate_US915_LoRa_SF7_500KHZ
@ LoRaWAN_DataRate_US915_LoRa_SF7_500KHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:121
LoRaWAN_Channel_US_DN_923_3_MHz_9
@ LoRaWAN_Channel_US_DN_923_3_MHz_9
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:473
LoRaWAN_Channel_US_DN_923_3_MHz_5
@ LoRaWAN_Channel_US_DN_923_3_MHz_5
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:437
LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_2
@ LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_2
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:120
LoRaWAN_Channel_US_UP_908_7_MHZ
@ LoRaWAN_Channel_US_UP_908_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:350
LoRaWAN_Channel_US_UP_909_5_MHZ
@ LoRaWAN_Channel_US_UP_909_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:354
LoRaWAN_Channel_US_UP_912_7_MHZ
@ LoRaWAN_Channel_US_UP_912_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:372
LoRaWAN_Channel_US_DN_927_5_MHz_4
@ LoRaWAN_Channel_US_DN_927_5_MHz_4
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:435
LoRaWAN_Channel_US_UP_908_5_MHZ
@ LoRaWAN_Channel_US_UP_908_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:348
LoRaWAN_Channel_US_DN_923_9_MHz_3
@ LoRaWAN_Channel_US_DN_923_9_MHz_3
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:420
LoRaWAN_Channel_US_UP_906_5_MHZ
@ LoRaWAN_Channel_US_UP_906_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:337
LoRaWAN_Channel_US_DN_926_9_MHz
@ LoRaWAN_Channel_US_DN_926_9_MHz
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:407
LoRaWAN_Channel_US_UP_903_0_MHZ
@ LoRaWAN_Channel_US_UP_903_0_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:386
LoRaWAN_Channel_US_DN_923_3_MHz_7
@ LoRaWAN_Channel_US_DN_923_3_MHz_7
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:455
LoRaWAN_Channel_US_DN_926_3_MHz
@ LoRaWAN_Channel_US_DN_926_3_MHz
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:406
LoRaWAN_Channel_US_DN_924_5_MHz_3
@ LoRaWAN_Channel_US_DN_924_5_MHz_3
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:421
LoRaWAN_Channel_US_DN_925_7_MHz_5
@ LoRaWAN_Channel_US_DN_925_7_MHz_5
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:441
LoRaWAN_Channel_US_DN_927_5_MHz_9
@ LoRaWAN_Channel_US_DN_927_5_MHz_9
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:480
LoRaWAN_Channel_US_UP_913_5_MHZ
@ LoRaWAN_Channel_US_UP_913_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:377
LoRaWAN_Channel_US_UP_905_9_MHZ
@ LoRaWAN_Channel_US_UP_905_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:334
LoRaWAN_Channel_US_DN_924_5_MHz
@ LoRaWAN_Channel_US_DN_924_5_MHz
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:403
LoRaWAN_Channel_US_UP_912_3_MHZ
@ LoRaWAN_Channel_US_UP_912_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:370
LoRaWAN_Channel_US_DN_925_7_MHz_6
@ LoRaWAN_Channel_US_DN_925_7_MHz_6
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:450
LoRaWAN_Channel_US_DN_925_1_MHz_4
@ LoRaWAN_Channel_US_DN_925_1_MHz_4
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:431
LoRaWAN_Channel_US_DN_927_5_MHz_7
@ LoRaWAN_Channel_US_DN_927_5_MHz_7
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:462
LoRaWAN_Channel_US_DN_924_5_MHz_9
@ LoRaWAN_Channel_US_DN_924_5_MHz_9
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:475
LoRaWAN_Channel_US_DN_923_3_MHz
@ LoRaWAN_Channel_US_DN_923_3_MHz
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:401
LoRaWAN_DataRate_US915_LoRa_SF12_500KHZ
@ LoRaWAN_DataRate_US915_LoRa_SF12_500KHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:116
TLoRaWAN_Channel_US_UP
TLoRaWAN_Channel_US_UP
Channel definition for US 915MHz Band uplink.
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:312
LoRaWAN_Channel_US_DN_927_5_MHz
@ LoRaWAN_Channel_US_DN_927_5_MHz
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:408
LoRaWAN_Channel_US_UP_913_1_MHZ
@ LoRaWAN_Channel_US_UP_913_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:374
LoRaWAN_Channel_US_DN_923_9_MHz_2
@ LoRaWAN_Channel_US_DN_923_9_MHz_2
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:411
LoRaWAN_DataRate_US915_LoRa_SF9_125KHZ
@ LoRaWAN_DataRate_US915_LoRa_SF9_125KHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:112
LoRaWAN_Channel_US_UP_903_9_MHZ
@ LoRaWAN_Channel_US_UP_903_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:323
LoRaWAN_Channel_US_DN_925_1_MHz_3
@ LoRaWAN_Channel_US_DN_925_1_MHz_3
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:422
LoRaWAN_Channel_US_UP_906_7_MHZ
@ LoRaWAN_Channel_US_UP_906_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:338
LoRaWAN_Channel_US_DN_927_5_MHz_6
@ LoRaWAN_Channel_US_DN_927_5_MHz_6
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:453
LoRaWAN_Channel_US_DN_923_9_MHz_4
@ LoRaWAN_Channel_US_DN_923_9_MHz_4
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:429
LoRaWAN_Channel_US_UP_903_1_MHZ
@ LoRaWAN_Channel_US_UP_903_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:318
LoRaWAN_Channel_US_UP_914_1_MHZ
@ LoRaWAN_Channel_US_UP_914_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:380
LoRaWAN_Channel_US_DN_926_3_MHz_3
@ LoRaWAN_Channel_US_DN_926_3_MHz_3
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:424
LoRaWAN_Channel_US_UP_911_7_MHZ
@ LoRaWAN_Channel_US_UP_911_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:366
TLoRaWAN_Channel_US_DN
TLoRaWAN_Channel_US_DN
Channel definition for US 915MHz Band downlink.
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:399
LoRaWAN_Channel_US_DN_927_5_MHz_3
@ LoRaWAN_Channel_US_DN_927_5_MHz_3
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:426
LoRaWAN_Channel_US_DN_925_1_MHz
@ LoRaWAN_Channel_US_DN_925_1_MHz
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:404
LoRaWAN_Channel_US_DN_925_1_MHz_9
@ LoRaWAN_Channel_US_DN_925_1_MHz_9
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:476
LoRaWAN_Channel_US_UP_907_8_MHZ
@ LoRaWAN_Channel_US_UP_907_8_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:389
LoRaWAN_Channel_US_DN_926_3_MHz_2
@ LoRaWAN_Channel_US_DN_926_3_MHz_2
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:415
LoRaWAN_Channel_US_UP_910_1_MHZ
@ LoRaWAN_Channel_US_UP_910_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:357
LoRaWAN_DataRate_US915_LoRa_SF8_125KHZ
@ LoRaWAN_DataRate_US915_LoRa_SF8_125KHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:113
LoRaWAN_Channel_US_UP_903_7_MHZ
@ LoRaWAN_Channel_US_UP_903_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:321
LoRaWAN_Channel_US_DN_924_5_MHz_8
@ LoRaWAN_Channel_US_DN_924_5_MHz_8
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:466
LoRaWAN_Channel_US_DN_923_3_MHz_4
@ LoRaWAN_Channel_US_DN_923_3_MHz_4
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:428
LoRaWAN_Channel_US_UP_909_4_MHZ
@ LoRaWAN_Channel_US_UP_909_4_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:390
LoRaWAN_Channel_US_UP_905_3_MHZ
@ LoRaWAN_Channel_US_UP_905_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:330
LoRaWAN_Channel_US_UP_913_7_MHZ
@ LoRaWAN_Channel_US_UP_913_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:378
LoRaWAN_Channel_US_DN_923_3_MHz_3
@ LoRaWAN_Channel_US_DN_923_3_MHz_3
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:419
LoRaWAN_Channel_US_DN_924_5_MHz_2
@ LoRaWAN_Channel_US_DN_924_5_MHz_2
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:412
LoRaWAN_Channel_US_DN_926_9_MHz_9
@ LoRaWAN_Channel_US_DN_926_9_MHz_9
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:479
LoRaWAN_Channel_US_UP_903_5_MHZ
@ LoRaWAN_Channel_US_UP_903_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:320
LoRaWAN_Channel_US_UP_906_2_MHZ
@ LoRaWAN_Channel_US_UP_906_2_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:388
LoRaWAN_Channel_US_DN_925_1_MHz_8
@ LoRaWAN_Channel_US_DN_925_1_MHz_8
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:467
LoRaWAN_Channel_US_UP_904_1_MHZ
@ LoRaWAN_Channel_US_UP_904_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:324
LoRaWAN_Channel_US_UP_910_5_MHZ
@ LoRaWAN_Channel_US_UP_910_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:360
LoRaWAN_Channel_US_DN_926_3_MHz_9
@ LoRaWAN_Channel_US_DN_926_3_MHz_9
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:478
LoRaWAN_Channel_US_DN_923_9_MHz_7
@ LoRaWAN_Channel_US_DN_923_9_MHz_7
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:456
LoRaWAN_Channel_US_DN_925_7_MHz_7
@ LoRaWAN_Channel_US_DN_925_7_MHz_7
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:459
LoRaWAN_Channel_US_UP_905_5_MHZ
@ LoRaWAN_Channel_US_UP_905_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:332
LoRaWAN_Channel_US_UP_914_7_MHZ
@ LoRaWAN_Channel_US_UP_914_7_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:383
LoRaWAN_Channel_US_DN_925_7_MHz_8
@ LoRaWAN_Channel_US_DN_925_7_MHz_8
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:468
LoRaWAN_Channel_US_DN_925_7_MHz_9
@ LoRaWAN_Channel_US_DN_925_7_MHz_9
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:477
LoRaWAN_Channel_US_DN_925_7_MHz_3
@ LoRaWAN_Channel_US_DN_925_7_MHz_3
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:423
LoRaWAN_Channel_US_DN_927_5_MHz_8
@ LoRaWAN_Channel_US_DN_927_5_MHz_8
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:471
LoRaWAN_Channel_US_DN_926_9_MHz_5
@ LoRaWAN_Channel_US_DN_926_9_MHz_5
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:443
LoRaWAN_Channel_US_DN_924_5_MHz_7
@ LoRaWAN_Channel_US_DN_924_5_MHz_7
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:457
LoRaWAN_DataRate_US915_LoRa_SF10_125KHZ
@ LoRaWAN_DataRate_US915_LoRa_SF10_125KHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:111
LoRaWAN_Channel_US_UP_907_5_MHZ
@ LoRaWAN_Channel_US_UP_907_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:343
LoRaWAN_Channel_US_DN_926_3_MHz_6
@ LoRaWAN_Channel_US_DN_926_3_MHz_6
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:451
LoRaWAN_Channel_US_DN_923_3_MHz_10
@ LoRaWAN_Channel_US_DN_923_3_MHz_10
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:482
LoRaWAN_Channel_US_UP_914_2_MHZ
@ LoRaWAN_Channel_US_UP_914_2_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:393
LoRaWAN_Channel_US_DN_926_3_MHz_5
@ LoRaWAN_Channel_US_DN_926_3_MHz_5
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:442
LoRaWAN_Channel_US_DN_926_9_MHz_6
@ LoRaWAN_Channel_US_DN_926_9_MHz_6
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:452
LoRaWAN_Channel_US_UP_912_5_MHZ
@ LoRaWAN_Channel_US_UP_912_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:371
LoRaWAN_Channel_US_UP_904_9_MHZ
@ LoRaWAN_Channel_US_UP_904_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:328
LoRaWAN_Channel_US_UP_904_3_MHZ
@ LoRaWAN_Channel_US_UP_904_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:325
LoRaWAN_Channel_US_UP_902_3_MHZ
@ LoRaWAN_Channel_US_UP_902_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:314
LoRaWAN_Channel_US_UP_904_6_MHZ
@ LoRaWAN_Channel_US_UP_904_6_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:387
LoRaWAN_Channel_US_UP_906_3_MHZ
@ LoRaWAN_Channel_US_UP_906_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:336
LoRaWAN_Channel_US_UP_907_3_MHZ
@ LoRaWAN_Channel_US_UP_907_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:342
LoRaWAN_DataRate_US915_LoRa_SF9_500KHZ
@ LoRaWAN_DataRate_US915_LoRa_SF9_500KHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:119
LoRaWAN_Channel_US_UP_905_1_MHZ
@ LoRaWAN_Channel_US_UP_905_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:329
LoRaWAN_Channel_US_DN_925_1_MHz_6
@ LoRaWAN_Channel_US_DN_925_1_MHz_6
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:449
LoRaWAN_Channel_US_UP_911_9_MHZ
@ LoRaWAN_Channel_US_UP_911_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:368
LoRaWAN_Channel_US_UP_911_5_MHZ
@ LoRaWAN_Channel_US_UP_911_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:365
LoRaWAN_Channel_US_UP_909_3_MHZ
@ LoRaWAN_Channel_US_UP_909_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:353
LoRaWAN_Channel_US_DN_923_9_MHz_5
@ LoRaWAN_Channel_US_DN_923_9_MHz_5
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:438
LoRaWAN_Channel_US_DN_927_5_MHz_5
@ LoRaWAN_Channel_US_DN_927_5_MHz_5
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:444
LoRaWAN_Channel_US_DN_923_9_MHz
@ LoRaWAN_Channel_US_DN_923_9_MHz
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:402
LoRaWAN_Channel_US_UP_913_9_MHZ
@ LoRaWAN_Channel_US_UP_913_9_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:379
LoRaWAN_Channel_US_UP_907_1_MHZ
@ LoRaWAN_Channel_US_UP_907_1_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:341
LoRaWAN_Channel_US_UP_914_3_MHZ
@ LoRaWAN_Channel_US_UP_914_3_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:381
LoRaWAN_Channel_US_UP_902_5_MHZ
@ LoRaWAN_Channel_US_UP_902_5_MHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:315
LoRaWAN_Channel_US_DN_923_9_MHz_6
@ LoRaWAN_Channel_US_DN_923_9_MHz_6
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:447
LoRaWAN_DataRate_US915_LoRa_SF7_125KHZ
@ LoRaWAN_DataRate_US915_LoRa_SF7_125KHZ
Definition: WiMOD_SAP_LORAWAN_IDs_US915.h:114