| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Typedefs | Enumerations
WiMOD_SAP_LORAWAN_IDs_US915.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Typedefs
typedef enum TLoRaWANDataRateUS915 | TLoRaWANDataRateUS915
| LoRa data rate definitions for US 915 MHz Band.
typedef enum TLoRaWAN_Channel_US_UP | TLoRaWAN_Channel_US_UP
| Channel definition for US 915MHz Band uplink.
typedef enum TLoRaWAN_Channel_US_DN | TLoRaWAN_Channel_US_DN
| Channel definition for US 915MHz Band downlink.

## Enumerations
enum | TLoRaWANDataRateUS915 { LoRaWAN_DataRate_US915_LoRa_SF10_125KHZ = 0, LoRaWAN_DataRate_US915_LoRa_SF9_125KHZ = 1, LoRaWAN_DataRate_US915_LoRa_SF8_125KHZ = 2, LoRaWAN_DataRate_US915_LoRa_SF7_125KHZ = 3, LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_1 = 4, LoRaWAN_DataRate_US915_LoRa_SF12_500KHZ = 8, LoRaWAN_DataRate_US915_LoRa_SF11_500KHZ = 9, LoRaWAN_DataRate_US915_LoRa_SF10_500KHZ = 10, LoRaWAN_DataRate_US915_LoRa_SF9_500KHZ = 11, LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_2 = 12, LoRaWAN_DataRate_US915_LoRa_SF7_500KHZ = 13 }
| LoRa data rate definitions for US 915 MHz Band. More...
enum | TLoRaWAN_Channel_US_UP { LoRaWAN_Channel_US_UP_902_3_MHZ = 0, LoRaWAN_Channel_US_UP_902_5_MHZ = 1, LoRaWAN_Channel_US_UP_902_7_MHZ = 2, LoRaWAN_Channel_US_UP_902_9_MHZ = 3, LoRaWAN_Channel_US_UP_903_1_MHZ = 4, LoRaWAN_Channel_US_UP_903_3_MHZ = 5, LoRaWAN_Channel_US_UP_903_5_MHZ = 6, LoRaWAN_Channel_US_UP_903_7_MHZ = 7, LoRaWAN_Channel_US_UP_903_9_MHZ = 8, LoRaWAN_Channel_US_UP_904_1_MHZ = 9, LoRaWAN_Channel_US_UP_904_3_MHZ = 10, LoRaWAN_Channel_US_UP_904_5_MHZ = 11, LoRaWAN_Channel_US_UP_904_7_MHZ = 12, LoRaWAN_Channel_US_UP_904_9_MHZ = 13, LoRaWAN_Channel_US_UP_905_1_MHZ = 14, LoRaWAN_Channel_US_UP_905_3_MHZ = 15, LoRaWAN_Channel_US_UP_905_5_MHZ = 16, LoRaWAN_Channel_US_UP_905_7_MHZ = 17, LoRaWAN_Channel_US_UP_905_9_MHZ = 18, LoRaWAN_Channel_US_UP_906_1_MHZ = 19, LoRaWAN_Channel_US_UP_906_3_MHZ = 20, LoRaWAN_Channel_US_UP_906_5_MHZ = 21, LoRaWAN_Channel_US_UP_906_7_MHZ = 22, LoRaWAN_Channel_US_UP_906_9_MHZ = 23, LoRaWAN_Channel_US_UP_907_1_MHZ = 24, LoRaWAN_Channel_US_UP_907_3_MHZ = 25, LoRaWAN_Channel_US_UP_907_5_MHZ = 26, LoRaWAN_Channel_US_UP_907_7_MHZ = 27, LoRaWAN_Channel_US_UP_907_9_MHZ = 28, LoRaWAN_Channel_US_UP_908_1_MHZ = 29, LoRaWAN_Channel_US_UP_908_3_MHZ = 30, LoRaWAN_Channel_US_UP_908_5_MHZ = 31, LoRaWAN_Channel_US_UP_908_7_MHZ = 32, LoRaWAN_Channel_US_UP_908_9_MHZ = 33, LoRaWAN_Channel_US_UP_909_1_MHZ = 34, LoRaWAN_Channel_US_UP_909_3_MHZ = 35, LoRaWAN_Channel_US_UP_909_5_MHZ = 36, LoRaWAN_Channel_US_UP_909_7_MHZ = 37, LoRaWAN_Channel_US_UP_909_9_MHZ = 38, LoRaWAN_Channel_US_UP_910_1_MHZ = 39, LoRaWAN_Channel_US_UP_910_3_MHZ = 40, LoRaWAN_Channel_US_UP_910_5_MHZ = 41, LoRaWAN_Channel_US_UP_910_7_MHZ = 42, LoRaWAN_Channel_US_UP_910_9_MHZ = 43, LoRaWAN_Channel_US_UP_911_1_MHZ = 44, LoRaWAN_Channel_US_UP_911_3_MHZ = 45, LoRaWAN_Channel_US_UP_911_5_MHZ = 46, LoRaWAN_Channel_US_UP_911_7_MHZ = 47, LoRaWAN_Channel_US_UP_911_9_MHZ = 48, LoRaWAN_Channel_US_UP_912_1_MHZ = 49, LoRaWAN_Channel_US_UP_912_3_MHZ = 50, LoRaWAN_Channel_US_UP_912_5_MHZ = 51, LoRaWAN_Channel_US_UP_912_7_MHZ = 52, LoRaWAN_Channel_US_UP_912_9_MHZ = 53, LoRaWAN_Channel_US_UP_913_1_MHZ = 54, LoRaWAN_Channel_US_UP_913_3_MHZ = 55, LoRaWAN_Channel_US_UP_913_5_MHZ = 56, LoRaWAN_Channel_US_UP_913_7_MHZ = 57, LoRaWAN_Channel_US_UP_913_9_MHZ = 58, LoRaWAN_Channel_US_UP_914_1_MHZ = 59, LoRaWAN_Channel_US_UP_914_3_MHZ = 60, LoRaWAN_Channel_US_UP_914_5_MHZ = 61, LoRaWAN_Channel_US_UP_914_7_MHZ = 62, LoRaWAN_Channel_US_UP_914_9_MHZ = 63, LoRaWAN_Channel_US_UP_903_0_MHZ = 64, LoRaWAN_Channel_US_UP_904_6_MHZ = 65, LoRaWAN_Channel_US_UP_906_2_MHZ = 66, LoRaWAN_Channel_US_UP_907_8_MHZ = 67, LoRaWAN_Channel_US_UP_909_4_MHZ = 68, LoRaWAN_Channel_US_UP_911_0_MHZ = 69, LoRaWAN_Channel_US_UP_912_6_MHZ = 70, LoRaWAN_Channel_US_UP_914_2_MHZ = 71 }
| Channel definition for US 915MHz Band uplink. More...
enum | TLoRaWAN_Channel_US_DN { LoRaWAN_Channel_US_DN_923_3_MHz = 0, LoRaWAN_Channel_US_DN_923_9_MHz = 1, LoRaWAN_Channel_US_DN_924_5_MHz = 2, LoRaWAN_Channel_US_DN_925_1_MHz = 3, LoRaWAN_Channel_US_DN_925_7_MHz = 4, LoRaWAN_Channel_US_DN_926_3_MHz = 5, LoRaWAN_Channel_US_DN_926_9_MHz = 6, LoRaWAN_Channel_US_DN_927_5_MHz = 7, LoRaWAN_Channel_US_DN_923_3_MHz_2 = 8, LoRaWAN_Channel_US_DN_923_9_MHz_2 = 9, LoRaWAN_Channel_US_DN_924_5_MHz_2 = 10, LoRaWAN_Channel_US_DN_925_1_MHz_2 = 11, LoRaWAN_Channel_US_DN_925_7_MHz_2 = 12, LoRaWAN_Channel_US_DN_926_3_MHz_2 = 13, LoRaWAN_Channel_US_DN_926_9_MHz_2 = 14, LoRaWAN_Channel_US_DN_927_5_MHz_2 = 15, LoRaWAN_Channel_US_DN_923_3_MHz_3 = 16, LoRaWAN_Channel_US_DN_923_9_MHz_3 = 17, LoRaWAN_Channel_US_DN_924_5_MHz_3 = 18, LoRaWAN_Channel_US_DN_925_1_MHz_3 = 19, LoRaWAN_Channel_US_DN_925_7_MHz_3 = 20, LoRaWAN_Channel_US_DN_926_3_MHz_3 = 21, LoRaWAN_Channel_US_DN_926_9_MHz_3 = 22, LoRaWAN_Channel_US_DN_927_5_MHz_3 = 23, LoRaWAN_Channel_US_DN_923_3_MHz_4 = 24, LoRaWAN_Channel_US_DN_923_9_MHz_4 = 25, LoRaWAN_Channel_US_DN_924_5_MHz_4 = 26, LoRaWAN_Channel_US_DN_925_1_MHz_4 = 27, LoRaWAN_Channel_US_DN_925_7_MHz_4 = 28, LoRaWAN_Channel_US_DN_926_3_MHz_4 = 29, LoRaWAN_Channel_US_DN_926_9_MHz_4 = 30, LoRaWAN_Channel_US_DN_927_5_MHz_4 = 31, LoRaWAN_Channel_US_DN_923_3_MHz_5 = 32, LoRaWAN_Channel_US_DN_923_9_MHz_5 = 33, LoRaWAN_Channel_US_DN_924_5_MHz_5 = 34, LoRaWAN_Channel_US_DN_925_1_MHz_5 = 35, LoRaWAN_Channel_US_DN_925_7_MHz_5 = 36, LoRaWAN_Channel_US_DN_926_3_MHz_5 = 37, LoRaWAN_Channel_US_DN_926_9_MHz_5 = 38, LoRaWAN_Channel_US_DN_927_5_MHz_5 = 39, LoRaWAN_Channel_US_DN_923_3_MHz_6 = 40, LoRaWAN_Channel_US_DN_923_9_MHz_6 = 41, LoRaWAN_Channel_US_DN_924_5_MHz_6 = 42, LoRaWAN_Channel_US_DN_925_1_MHz_6 = 43, LoRaWAN_Channel_US_DN_925_7_MHz_6 = 44, LoRaWAN_Channel_US_DN_926_3_MHz_6 = 45, LoRaWAN_Channel_US_DN_926_9_MHz_6 = 46, LoRaWAN_Channel_US_DN_927_5_MHz_6 = 47, LoRaWAN_Channel_US_DN_923_3_MHz_7 = 48, LoRaWAN_Channel_US_DN_923_9_MHz_7 = 49, LoRaWAN_Channel_US_DN_924_5_MHz_7 = 50, LoRaWAN_Channel_US_DN_925_1_MHz_7 = 51, LoRaWAN_Channel_US_DN_925_7_MHz_7 = 52, LoRaWAN_Channel_US_DN_926_3_MHz_7 = 53, LoRaWAN_Channel_US_DN_926_9_MHz_7 = 54, LoRaWAN_Channel_US_DN_927_5_MHz_7 = 55, LoRaWAN_Channel_US_DN_923_3_MHz_8 = 56, LoRaWAN_Channel_US_DN_923_9_MHz_8 = 57, LoRaWAN_Channel_US_DN_924_5_MHz_8 = 58, LoRaWAN_Channel_US_DN_925_1_MHz_8 = 59, LoRaWAN_Channel_US_DN_925_7_MHz_8 = 60, LoRaWAN_Channel_US_DN_926_3_MHz_8 = 61, LoRaWAN_Channel_US_DN_926_9_MHz_8 = 62, LoRaWAN_Channel_US_DN_927_5_MHz_8 = 63, LoRaWAN_Channel_US_DN_923_3_MHz_9 = 64, LoRaWAN_Channel_US_DN_923_9_MHz_9 = 65, LoRaWAN_Channel_US_DN_924_5_MHz_9 = 66, LoRaWAN_Channel_US_DN_925_1_MHz_9 = 67, LoRaWAN_Channel_US_DN_925_7_MHz_9 = 68, LoRaWAN_Channel_US_DN_926_3_MHz_9 = 69, LoRaWAN_Channel_US_DN_926_9_MHz_9 = 70, LoRaWAN_Channel_US_DN_927_5_MHz_9 = 71, LoRaWAN_Channel_US_DN_923_3_MHz_10 = 128 }
| Channel definition for US 915MHz Band downlink. More...

## Enumeration Type Documentation

## ◆ TLoRaWAN_Channel_US_DN

enum TLoRaWAN_Channel_US_DN

Channel definition for US 915MHz Band downlink.

Enumerator
LoRaWAN_Channel_US_DN_923_3_MHz | carrier frequency of 923.3 MHz for downlink
LoRaWAN_Channel_US_DN_923_9_MHz | carrier frequency of 923.9 MHz for downlink
LoRaWAN_Channel_US_DN_924_5_MHz | carrier frequency of 924.5 MHz for downlink
LoRaWAN_Channel_US_DN_925_1_MHz | carrier frequency of 925.1 MHz for downlink
LoRaWAN_Channel_US_DN_925_7_MHz | carrier frequency of 925.7 MHz for downlink
LoRaWAN_Channel_US_DN_926_3_MHz | carrier frequency of 926.3 MHz for downlink
LoRaWAN_Channel_US_DN_926_9_MHz | carrier frequency of 926.9 MHz for downlink
LoRaWAN_Channel_US_DN_927_5_MHz | carrier frequency of 927.5 MHz for downlink
LoRaWAN_Channel_US_DN_923_3_MHz_2 | carrier frequency of 923.3 MHz for downlink
LoRaWAN_Channel_US_DN_923_9_MHz_2 | carrier frequency of 923.9 MHz for downlink
LoRaWAN_Channel_US_DN_924_5_MHz_2 | carrier frequency of 924.5 MHz for downlink
LoRaWAN_Channel_US_DN_925_1_MHz_2 | carrier frequency of 925.1 MHz for downlink
LoRaWAN_Channel_US_DN_925_7_MHz_2 | carrier frequency of 925.7 MHz for downlink
LoRaWAN_Channel_US_DN_926_3_MHz_2 | carrier frequency of 926.3 MHz for downlink
LoRaWAN_Channel_US_DN_926_9_MHz_2 | carrier frequency of 926.9 MHz for downlink
LoRaWAN_Channel_US_DN_927_5_MHz_2 | carrier frequency of 927.5 MHz for downlink
LoRaWAN_Channel_US_DN_923_3_MHz_3 | carrier frequency of 923.3 MHz for downlink
LoRaWAN_Channel_US_DN_923_9_MHz_3 | carrier frequency of 923.9 MHz for downlink
LoRaWAN_Channel_US_DN_924_5_MHz_3 | carrier frequency of 924.5 MHz for downlink
LoRaWAN_Channel_US_DN_925_1_MHz_3 | carrier frequency of 925.1 MHz for downlink
LoRaWAN_Channel_US_DN_925_7_MHz_3 | carrier frequency of 925.7 MHz for downlink
LoRaWAN_Channel_US_DN_926_3_MHz_3 | carrier frequency of 926.3 MHz for downlink
LoRaWAN_Channel_US_DN_926_9_MHz_3 | carrier frequency of 926.9 MHz for downlink
LoRaWAN_Channel_US_DN_927_5_MHz_3 | carrier frequency of 927.5 MHz for downlink
LoRaWAN_Channel_US_DN_923_3_MHz_4 | carrier frequency of 923.3 MHz for downlink
LoRaWAN_Channel_US_DN_923_9_MHz_4 | carrier frequency of 923.9 MHz for downlink
LoRaWAN_Channel_US_DN_924_5_MHz_4 | carrier frequency of 924.5 MHz for downlink
LoRaWAN_Channel_US_DN_925_1_MHz_4 | carrier frequency of 925.1 MHz for downlink
LoRaWAN_Channel_US_DN_925_7_MHz_4 | carrier frequency of 925.7 MHz for downlink
LoRaWAN_Channel_US_DN_926_3_MHz_4 | carrier frequency of 926.3 MHz for downlink
LoRaWAN_Channel_US_DN_926_9_MHz_4 | carrier frequency of 926.9 MHz for downlink
LoRaWAN_Channel_US_DN_927_5_MHz_4 | carrier frequency of 927.5 MHz for downlink
LoRaWAN_Channel_US_DN_923_3_MHz_5 | carrier frequency of 923.3 MHz for downlink
LoRaWAN_Channel_US_DN_923_9_MHz_5 | carrier frequency of 923.9 MHz for downlink
LoRaWAN_Channel_US_DN_924_5_MHz_5 | carrier frequency of 924.5 MHz for downlink
LoRaWAN_Channel_US_DN_925_1_MHz_5 | carrier frequency of 925.1 MHz for downlink
LoRaWAN_Channel_US_DN_925_7_MHz_5 | carrier frequency of 925.7 MHz for downlink
LoRaWAN_Channel_US_DN_926_3_MHz_5 | carrier frequency of 926.3 MHz for downlink
LoRaWAN_Channel_US_DN_926_9_MHz_5 | carrier frequency of 926.9 MHz for downlink
LoRaWAN_Channel_US_DN_927_5_MHz_5 | carrier frequency of 927.5 MHz for downlink
LoRaWAN_Channel_US_DN_923_3_MHz_6 | carrier frequency of 923.3 MHz for downlink
LoRaWAN_Channel_US_DN_923_9_MHz_6 | carrier frequency of 923.9 MHz for downlink
LoRaWAN_Channel_US_DN_924_5_MHz_6 | carrier frequency of 924.5 MHz for downlink
LoRaWAN_Channel_US_DN_925_1_MHz_6 | carrier frequency of 925.1 MHz for downlink
LoRaWAN_Channel_US_DN_925_7_MHz_6 | carrier frequency of 925.7 MHz for downlink
LoRaWAN_Channel_US_DN_926_3_MHz_6 | carrier frequency of 926.3 MHz for downlink
LoRaWAN_Channel_US_DN_926_9_MHz_6 | carrier frequency of 926.9 MHz for downlink
LoRaWAN_Channel_US_DN_927_5_MHz_6 | carrier frequency of 927.5 MHz for downlink
LoRaWAN_Channel_US_DN_923_3_MHz_7 | carrier frequency of 923.3 MHz for downlink
LoRaWAN_Channel_US_DN_923_9_MHz_7 | carrier frequency of 923.9 MHz for downlink
LoRaWAN_Channel_US_DN_924_5_MHz_7 | carrier frequency of 924.5 MHz for downlink
LoRaWAN_Channel_US_DN_925_1_MHz_7 | carrier frequency of 925.1 MHz for downlink
LoRaWAN_Channel_US_DN_925_7_MHz_7 | carrier frequency of 925.7 MHz for downlink
LoRaWAN_Channel_US_DN_926_3_MHz_7 | carrier frequency of 926.3 MHz for downlink
LoRaWAN_Channel_US_DN_926_9_MHz_7 | carrier frequency of 926.9 MHz for downlink
LoRaWAN_Channel_US_DN_927_5_MHz_7 | carrier frequency of 927.5 MHz for downlink
LoRaWAN_Channel_US_DN_923_3_MHz_8 | carrier frequency of 923.3 MHz for downlink
LoRaWAN_Channel_US_DN_923_9_MHz_8 | carrier frequency of 923.9 MHz for downlink
LoRaWAN_Channel_US_DN_924_5_MHz_8 | carrier frequency of 924.5 MHz for downlink
LoRaWAN_Channel_US_DN_925_1_MHz_8 | carrier frequency of 925.1 MHz for downlink
LoRaWAN_Channel_US_DN_925_7_MHz_8 | carrier frequency of 925.7 MHz for downlink
LoRaWAN_Channel_US_DN_926_3_MHz_8 | carrier frequency of 926.3 MHz for downlink
LoRaWAN_Channel_US_DN_926_9_MHz_8 | carrier frequency of 926.9 MHz for downlink
LoRaWAN_Channel_US_DN_927_5_MHz_8 | carrier frequency of 927.5 MHz for downlink
LoRaWAN_Channel_US_DN_923_3_MHz_9 | carrier frequency of 923.3 MHz for downlink
LoRaWAN_Channel_US_DN_923_9_MHz_9 | carrier frequency of 923.9 MHz for downlink
LoRaWAN_Channel_US_DN_924_5_MHz_9 | carrier frequency of 924.5 MHz for downlink
LoRaWAN_Channel_US_DN_925_1_MHz_9 | carrier frequency of 925.1 MHz for downlink
LoRaWAN_Channel_US_DN_925_7_MHz_9 | carrier frequency of 925.7 MHz for downlink
LoRaWAN_Channel_US_DN_926_3_MHz_9 | carrier frequency of 926.3 MHz for downlink
LoRaWAN_Channel_US_DN_926_9_MHz_9 | carrier frequency of 926.9 MHz for downlink
LoRaWAN_Channel_US_DN_927_5_MHz_9 | carrier frequency of 927.5 MHz for downlink
LoRaWAN_Channel_US_DN_923_3_MHz_10 | carrier frequency of 923.3 MHz for downlink

## ◆ TLoRaWAN_Channel_US_UP

enum TLoRaWAN_Channel_US_UP

Channel definition for US 915MHz Band uplink.

Enumerator
LoRaWAN_Channel_US_UP_902_3_MHZ | carrier frequency of 902.3 MHz for uplink
LoRaWAN_Channel_US_UP_902_5_MHZ | carrier frequency of 902.5 MHz for uplink
LoRaWAN_Channel_US_UP_902_7_MHZ | carrier frequency of 902.7 MHz for uplink
LoRaWAN_Channel_US_UP_902_9_MHZ | carrier frequency of 902.9 MHz for uplink
LoRaWAN_Channel_US_UP_903_1_MHZ | carrier frequency of 903.1 MHz for uplink
LoRaWAN_Channel_US_UP_903_3_MHZ | carrier frequency of 903.3 MHz for uplink
LoRaWAN_Channel_US_UP_903_5_MHZ | carrier frequency of 903.5 MHz for uplink
LoRaWAN_Channel_US_UP_903_7_MHZ | carrier frequency of 903.7 MHz for uplink
LoRaWAN_Channel_US_UP_903_9_MHZ | carrier frequency of 903.9 MHz for uplink
LoRaWAN_Channel_US_UP_904_1_MHZ | carrier frequency of 904.1 MHz for uplink
LoRaWAN_Channel_US_UP_904_3_MHZ | carrier frequency of 904.3 MHz for uplink
LoRaWAN_Channel_US_UP_904_5_MHZ | carrier frequency of 904.5 MHz for uplink
LoRaWAN_Channel_US_UP_904_7_MHZ | carrier frequency of 904.7 MHz for uplink
LoRaWAN_Channel_US_UP_904_9_MHZ | carrier frequency of 904.9 MHz for uplink
LoRaWAN_Channel_US_UP_905_1_MHZ | carrier frequency of 905.1 MHz for uplink
LoRaWAN_Channel_US_UP_905_3_MHZ | carrier frequency of 905.3 MHz for uplink
LoRaWAN_Channel_US_UP_905_5_MHZ | carrier frequency of 905.5 MHz for uplink
LoRaWAN_Channel_US_UP_905_7_MHZ | carrier frequency of 905.7 MHz for uplink
LoRaWAN_Channel_US_UP_905_9_MHZ | carrier frequency of 905.9 MHz for uplink
LoRaWAN_Channel_US_UP_906_1_MHZ | carrier frequency of 906.1 MHz for uplink
LoRaWAN_Channel_US_UP_906_3_MHZ | carrier frequency of 906.3 MHz for uplink
LoRaWAN_Channel_US_UP_906_5_MHZ | carrier frequency of 906.5 MHz for uplink
LoRaWAN_Channel_US_UP_906_7_MHZ | carrier frequency of 906.7 MHz for uplink
LoRaWAN_Channel_US_UP_906_9_MHZ | carrier frequency of 906.9 MHz for uplink
LoRaWAN_Channel_US_UP_907_1_MHZ | carrier frequency of 907.1 MHz for uplink
LoRaWAN_Channel_US_UP_907_3_MHZ | carrier frequency of 907.3 MHz for uplink
LoRaWAN_Channel_US_UP_907_5_MHZ | carrier frequency of 907.5 MHz for uplink
LoRaWAN_Channel_US_UP_907_7_MHZ | carrier frequency of 907.7 MHz for uplink
LoRaWAN_Channel_US_UP_907_9_MHZ | carrier frequency of 907.9 MHz for uplink
LoRaWAN_Channel_US_UP_908_1_MHZ | carrier frequency of 908.1 MHz for uplink
LoRaWAN_Channel_US_UP_908_3_MHZ | carrier frequency of 908.3 MHz for uplink
LoRaWAN_Channel_US_UP_908_5_MHZ | carrier frequency of 908.5 MHz for uplink
LoRaWAN_Channel_US_UP_908_7_MHZ | carrier frequency of 908.7 MHz for uplink
LoRaWAN_Channel_US_UP_908_9_MHZ | carrier frequency of 908.9 MHz for uplink
LoRaWAN_Channel_US_UP_909_1_MHZ | carrier frequency of 909.1 MHz for uplink
LoRaWAN_Channel_US_UP_909_3_MHZ | carrier frequency of 909.3 MHz for uplink
LoRaWAN_Channel_US_UP_909_5_MHZ | carrier frequency of 909.5 MHz for uplink
LoRaWAN_Channel_US_UP_909_7_MHZ | carrier frequency of 909.7 MHz for uplink
LoRaWAN_Channel_US_UP_909_9_MHZ | carrier frequency of 909.9 MHz for uplink
LoRaWAN_Channel_US_UP_910_1_MHZ | carrier frequency of 910.1 MHz for uplink
LoRaWAN_Channel_US_UP_910_3_MHZ | carrier frequency of 910.3 MHz for uplink
LoRaWAN_Channel_US_UP_910_5_MHZ | carrier frequency of 910.5 MHz for uplink
LoRaWAN_Channel_US_UP_910_7_MHZ | carrier frequency of 910.7 MHz for uplink
LoRaWAN_Channel_US_UP_910_9_MHZ | carrier frequency of 910.9 MHz for uplink
LoRaWAN_Channel_US_UP_911_1_MHZ | carrier frequency of 911.1 MHz for uplink
LoRaWAN_Channel_US_UP_911_3_MHZ | carrier frequency of 911.3 MHz for uplink
LoRaWAN_Channel_US_UP_911_5_MHZ | carrier frequency of 911.5 MHz for uplink
LoRaWAN_Channel_US_UP_911_7_MHZ | carrier frequency of 911.7 MHz for uplink
LoRaWAN_Channel_US_UP_911_9_MHZ | carrier frequency of 911.9 MHz for uplink
LoRaWAN_Channel_US_UP_912_1_MHZ | carrier frequency of 912.1 MHz for uplink
LoRaWAN_Channel_US_UP_912_3_MHZ | carrier frequency of 912.3 MHz for uplink
LoRaWAN_Channel_US_UP_912_5_MHZ | carrier frequency of 912.5 MHz for uplink
LoRaWAN_Channel_US_UP_912_7_MHZ | carrier frequency of 912.7 MHz for uplink
LoRaWAN_Channel_US_UP_912_9_MHZ | carrier frequency of 912.9 MHz for uplink
LoRaWAN_Channel_US_UP_913_1_MHZ | carrier frequency of 913.1 MHz for uplink
LoRaWAN_Channel_US_UP_913_3_MHZ | carrier frequency of 913.3 MHz for uplink
LoRaWAN_Channel_US_UP_913_5_MHZ | carrier frequency of 913.5 MHz for uplink
LoRaWAN_Channel_US_UP_913_7_MHZ | carrier frequency of 913.7 MHz for uplink
LoRaWAN_Channel_US_UP_913_9_MHZ | carrier frequency of 913.9 MHz for uplink
LoRaWAN_Channel_US_UP_914_1_MHZ | carrier frequency of 914.1 MHz for uplink
LoRaWAN_Channel_US_UP_914_3_MHZ | carrier frequency of 914.3 MHz for uplink
LoRaWAN_Channel_US_UP_914_5_MHZ | carrier frequency of 914.5 MHz for uplink
LoRaWAN_Channel_US_UP_914_7_MHZ | carrier frequency of 914.7 MHz for uplink
LoRaWAN_Channel_US_UP_914_9_MHZ | carrier frequency of 914.9 MHz for uplink
LoRaWAN_Channel_US_UP_903_0_MHZ | carrier frequency of 903.0 MHz for uplink
LoRaWAN_Channel_US_UP_904_6_MHZ | carrier frequency of 904.6 MHz for uplink
LoRaWAN_Channel_US_UP_906_2_MHZ | carrier frequency of 906.2 MHz for uplink
LoRaWAN_Channel_US_UP_907_8_MHZ | carrier frequency of 907.8 MHz for uplink
LoRaWAN_Channel_US_UP_909_4_MHZ | carrier frequency of 909.4 MHz for uplink
LoRaWAN_Channel_US_UP_911_0_MHZ | carrier frequency of 911.0 MHz for uplink
LoRaWAN_Channel_US_UP_912_6_MHZ | carrier frequency of 912.6 MHz for uplink
LoRaWAN_Channel_US_UP_914_2_MHZ | carrier frequency of 914.2 MHz for uplink

## ◆ TLoRaWANDataRateUS915

enum TLoRaWANDataRateUS915

LoRa data rate definitions for US 915 MHz Band.

Enumerator
LoRaWAN_DataRate_US915_LoRa_SF10_125KHZ | LoRa Spreading factor 10 using 125kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF9_125KHZ | LoRa Spreading factor 9 using 125kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF8_125KHZ | LoRa Spreading factor 8 using 125kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF7_125KHZ | LoRa Spreading factor 7 using 125kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_1 | LoRa Spreading factor 8 using 500kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF12_500KHZ | LoRa Spreading factor 12 using 500kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF11_500KHZ | LoRa Spreading factor 11 using 500kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF10_500KHZ | LoRa Spreading factor 10 using 500kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF9_500KHZ | LoRa Spreading factor 9 using 500kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF8_500KHZ_2 | LoRa Spreading factor 8 using 500kHz bandwidth
LoRaWAN_DataRate_US915_LoRa_SF7_500KHZ | LoRa Spreading factor 7 using 500kHz bandwidth