| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLORAWAN_ActivateDeviceData Struct Reference

Activation data structure for LoRa network activation. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

Inheritance diagram for TWiMODLORAWAN_ActivateDeviceData:
[legend]

## Public Attributes
UINT32 | DeviceAddress
UINT8 | NwkSKey [WiMODLORAWAN_NWK_SESSION_KEY_LEN]
UINT8 | AppSKey [WiMODLORAWAN_APP_SESSION_KEY_LEN]

## Detailed Description

Activation data structure for LoRa network activation.

## Member Data Documentation

## ◆ AppSKey

UINT8 TWiMODLORAWAN_ActivateDeviceData::AppSKey[WiMODLORAWAN_APP_SESSION_KEY_LEN]

secret application session key (128bit)

## ◆ DeviceAddress

UINT32 TWiMODLORAWAN_ActivateDeviceData::DeviceAddress

address of the WiMOD within the LoRa network (pre-set for ABP; set by nwk if OTAA was used

## ◆ NwkSKey

UINT8 TWiMODLORAWAN_ActivateDeviceData::NwkSKey[WiMODLORAWAN_NWK_SESSION_KEY_LEN]

secret network session key (128bit)

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h