| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLORAWAN_McastConfig Struct Reference

## Public Attributes
UINT8 | MulticastIndex
UINT32 | DeviceAddress
UINT8 | MulticastStatus
UINT8 | NwkSKey [WiMODLORAWAN_NWK_SESSION_KEY_LEN]
UINT8 | AppSKey [WiMODLORAWAN_APP_SESSION_KEY_LEN]

## Member Data Documentation

## ◆ AppSKey

UINT8 TWiMODLORAWAN_McastConfig::AppSKey[WiMODLORAWAN_APP_SESSION_KEY_LEN]

secret application session key (128bit) for Multicast context

## ◆ DeviceAddress

UINT32 TWiMODLORAWAN_McastConfig::DeviceAddress

address of the WiMOD within the Multicast context of LoRaWAN network

## ◆ MulticastStatus

UINT8 TWiMODLORAWAN_McastConfig::MulticastStatus

Status of Multicast Mode; 1 = active

## ◆ NwkSKey

UINT8 TWiMODLORAWAN_McastConfig::NwkSKey[WiMODLORAWAN_NWK_SESSION_KEY_LEN]

secret network session key (128bit) for Multicast context

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_ProLink_IDs.h