| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Classes | Macros | Typedefs | Enumerations
WiMOD_SAP_DEVMGMT_ProLink_IDs.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Classes
struct | TProLinkDeviceConfig
struct | TProLinkDeviceStatus

## Macros
#define | PROLINK_DEVMGMT_MSG_GET_DEVICE_STATUS_REQ 0x17
#define | PROLINK_DEVMGMT_MSG_GET_DEVICE_STATUS_RSP 0x18
#define | PROLINK_DEVMGMT_MSG_SET_DEVICE_CONFIG_REQ 0x25
#define | PROLINK_DEVMGMT_MSG_SET_DEVICE_CONFIG_RSP 0x26
#define | PROLINK_DEVMGMT_MSG_GET_DEVICE_CONFIG_REQ 0x27
#define | PROLINK_DEVMGMT_MSG_GET_DEVICE_CONFIG_RSP 0x28
#define | PROLINK_DEVMGMT_MSG_RESET_DEVICE_CONFIG_REQ 0x29
#define | PROLINK_DEVMGMT_MSG_RESET_DEVICE_CONFIG_RSP 0x2A
#define | PROLINK_DEVMGMT_MSG_SET_RADIO_STACK_REQ 0x39
#define | PROLINK_DEVMGMT_MSG_SET_RADIO_STACK_RSP 0x3A
#define | PROLINK_DEVMGMT_MSG_GET_RADIO_STACK_REQ 0x3B
#define | PROLINK_DEVMGMT_MSG_GET_RADIO_STACK_RSP 0x3C
#define | PROLINK_DEVICE_CFG_MISC_HCI_PWR_UP_IND_ENABLED (1 << 3)

## Typedefs
typedef enum TRadioStack_Mode | TRadioStack_Mode
| Radio Stack Mode(only for ProLink)
typedef struct TProLinkDeviceConfig | TProLinkDeviceConfig
typedef struct TProLinkDeviceStatus | TProLinkDeviceStatus

## Enumerations
enum | TRadioStack_Mode { RadioStack_LoRaWAN = 0, RadioStack_PROPRIETARY_LR_BASE }
| Radio Stack Mode(only for ProLink) More...

## Enumeration Type Documentation

## ◆ TRadioStack_Mode

enum TRadioStack_Mode

Radio Stack Mode(only for ProLink)

Enumerator
RadioStack_LoRaWAN | LoRaWAN Stack Mode
RadioStack_PROPRIETARY_LR_BASE | proprietary LR BASE Stack Mode