| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

WiMODLoRaWAN Member List

This is the complete list of members for WiMODLoRaWAN, including all inherited members.

ActivateDevice(TWiMODLORAWAN_ActivateDeviceData &activationData, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
begin(TLoRaWANregion region=LoRaWAN_Region_EU868) | WiMODLoRaWAN |
TWiMODLRHCI::begin(void) | TWiMODLRHCI | virtual
ClearRtcAlarm(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
ConnectViaOTAA(const uint8_t *appEUI=NULL, const uint8_t *appKey=NULL) | WiMODLoRaWAN |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_Data *loraWanRxData) | WiMODLoRaWAN |
convert(TWiMODLR_HCIMessage &rxMsg, TWiMODLORAWAN_TxIndData *sendIndData) | WiMODLoRaWAN |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_MacCmdData *loraWanMacCmdData) | WiMODLoRaWAN |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_JoinedNwkData *joinedNwkData) | WiMODLoRaWAN |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_ACK_Data *ackData) | WiMODLoRaWAN |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_NoData_Data *info) | WiMODLoRaWAN |
ConvertAppEuiStrToArray(char *appEuiStr, uint8_t *appEuiArray) | WiMODLoRaWAN |
ConvertAppKeyStrToArray(char *appKeyStr, uint8_t *appKeyArray) | WiMODLoRaWAN |
ConvertAppSKeyStrToArray(char *appSKeyStr, uint8_t *appSKeyArray) | WiMODLoRaWAN |
ConvertNwkSKeyStrToArray(char *nwkSKeyStr, uint8_t *nwkSKeyArray) | WiMODLoRaWAN |
copyDevMgmtResultInfos(TWiMODLRResultCodes *hciResult, UINT8 *rspStatus) (defined in WiMODLoRaWAN) | WiMODLoRaWAN | protected
copyLoRaWanResultInfos(TWiMODLRResultCodes *hciResult, UINT8 *rspStatus) (defined in WiMODLoRaWAN) | WiMODLoRaWAN | protected
DeactivateDevice(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
EnableWakeupSequence(bool flag) (defined in TWiMODLRHCI) | TWiMODLRHCI |
end(void) | WiMODLoRaWAN | virtual
ExecuteGenericCmd(TWiMODLR_Generic_CmdInfo *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
FactoryReset(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetCustomConfig(INT8 *rfGain, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetDeviceEUI(UINT8 *deviceEUI, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetDeviceInfo(TWiMODLR_DevMgmt_DevInfoLoRaWan *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetFirmwareInfo(TWiMODLR_DevMgmt_FwInfo *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetHciConfig(TWiMODLR_DevMgmt_HciConfig *hciConfig, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetLastHciResult(void) | WiMODLoRaWAN |
GetLastResponseStatus(void) | WiMODLoRaWAN |
GetNwkStatus(TWiMODLORAWAN_NwkStatus_Data *nwkStatus, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetOperationMode(TWiMOD_OperationMode *opMode, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetRadioStackConfig(TWiMODLORAWAN_RadioStackConfig *data, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetRtc(UINT32 *rtcTime, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetRtcAlarm(TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetRxMessage(void) (defined in TWiMODLRHCI) | TWiMODLRHCI |
GetSupportedBands(TWiMODLORAWAN_SupportedBands *supportedBands, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetSystemStatus(TWiMODLR_DevMgmt_SystemStatusLorawan *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
GetTxPowerLimitConfig(TWiMODLORAWAN_TxPwrLimitConfig *txPwrLimitCfg, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
JoinNetwork(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
Ping(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
PostMessage(UINT8 sapID, UINT8 msgID, UINT8 *payload, UINT16 length) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
PrintBasicDeviceInfo(Stream &s) (defined in WiMODLoRaWAN) | WiMODLoRaWAN |
Process(void) | TWiMODLRHCI |
ProcessRxMessage(UINT8 *rxBuffer, UINT16 length) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
ProcessUnexpectedRxMessage(TWiMODLR_HCIMessage &rxMsg) (defined in WiMODLoRaWAN) | WiMODLoRaWAN | protected virtual
ReactivateDevice(UINT32 *devAdr, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
RegisterJoinedNwkIndicationClient(TJoinedNwkIndicationCallback cb) | WiMODLoRaWAN |
RegisterJoinTxIndicationClient(TJoinTxIndicationCallback cb) | WiMODLoRaWAN |
RegisterNoDataIndicationClient(TNoDataIndicationCallback cb) | WiMODLoRaWAN |
RegisterPowerUpIndicationClient(TDevMgmtPowerUpCallback cb) | WiMODLoRaWAN |
RegisterRtcAlarmIndicationClient(TDevMgmtRtcAlarmCallback cb) | WiMODLoRaWAN |
RegisterRxAckIndicationClient(TRxAckIndicationCallback cb) | WiMODLoRaWAN |
RegisterRxCDataIndicationClient(TRxCDataIndicationCallback cb) | WiMODLoRaWAN |
RegisterRxMacCmdIndicationClient(TRxMacCmdIndicationCallback cb) | WiMODLoRaWAN |
RegisterRxUDataIndicationClient(TRxUDataIndicationCallback cb) | WiMODLoRaWAN |
RegisterStackErrorClient(TWiMODStackErrorClient cb) (defined in TWiMODLRHCI) | TWiMODLRHCI |
RegisterTxCDataIndicationClient(TTxCDataIndicationCallback cb) | WiMODLoRaWAN |
RegisterTxUDataIndicationClient(TTxUDataIndicationCallback cb) | WiMODLoRaWAN |
Reset(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SapDevMgmt | WiMODLoRaWAN | protected
SapGeneric | WiMODLoRaWAN | protected
SapLoRaWan | WiMODLoRaWAN | protected
SendCData(const TWiMODLORAWAN_TX_Data *data, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SendHCIMessage(UINT8 dstSapID, UINT8 msgID, UINT8 rxMsgID, UINT8 *payload, UINT16 length) | TWiMODLRHCI |
SendHCIMessageWithoutRx(UINT8 dstSapID, UINT8 msgID, UINT8 *payload, UINT16 length) | TWiMODLRHCI |
SendMacCmd(const TWiMODLORAWAN_MacCmd *cmd, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SendPacket(UINT8 *txData, UINT16 length) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
SendUData(const TWiMODLORAWAN_TX_Data *data, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SendWakeUpSequence(void) | TWiMODLRHCI |
SetBatteryLevelStatus(UINT8 battStatus, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SetCustomConfig(const INT8 rfGain, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SetDeviceEUI(const UINT8 *deviceEUI, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SetHciConfig(TWiMODLR_DevMgmt_HciConfig &hciConfig, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SetJoinParameter(TWiMODLORAWAN_JoinParams &joinParams, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SetOperationMode(const TWiMOD_OperationMode opMode, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SetRadioStackConfig(TWiMODLORAWAN_RadioStackConfig *data, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SetRtc(const UINT32 rtcTime, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SetRtcAlarm(const TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
SetTxPowerLimitConfig(TWiMODLORAWAN_TxPwrLimitConfig &txPwrLimitCfg, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLoRaWAN |
TComSlipClient() (defined in TComSlipClient) | TComSlipClient | inline
TWiMODLRHCI(Stream &s) | TWiMODLRHCI |
WaitForResponse(UINT8 rxSapID, UINT8 rxMsgID) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
WiMODLoRaWAN(Stream &s) | WiMODLoRaWAN |
~TComSlipClient() (defined in TComSlipClient) | TComSlipClient | inline virtual
~TWiMODLRHCI(void) | TWiMODLRHCI |
~WiMODLoRaWAN(void) | WiMODLoRaWAN |