| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODProLinkLORAWAN_RadioStackConfig Struct Reference

Radio stack configuration related to to LoRaWAN specific options. More...

`#include <SAP/WiMOD_SAP_LORAWAN_ProLink_IDs.h>`

## Public Attributes
UINT8 | DataRateIndex
UINT8 | TXPowerLevel
UINT8 | Options
UINT8 | Retransmissions
UINT8 | BandIndex
UINT8 | HeaderMacCmdCapacity
UINT8 | SubBandMask1
UINT8 | SubBandMask2
UINT8 | WrongParamErrCode

## Detailed Description

Radio stack configuration related to to LoRaWAN specific options.

## Member Data Documentation

## ◆ BandIndex

UINT8 TWiMODProLinkLORAWAN_RadioStackConfig::BandIndex

Frequency band to use (

See also
  TLoRaWAN_FreqBand)

## ◆ DataRateIndex

UINT8 TWiMODProLinkLORAWAN_RadioStackConfig::DataRateIndex

data rate to use (

See also
  TLoRaWANDataRate*)

## ◆ HeaderMacCmdCapacity

UINT8 TWiMODProLinkLORAWAN_RadioStackConfig::HeaderMacCmdCapacity

Header MAC Cmd Capatity (size in Byte)

## ◆ Options

UINT8 TWiMODProLinkLORAWAN_RadioStackConfig::Options

misc Options (see LORAWAN_STK_OPTION defines)

## ◆ Retransmissions

UINT8 TWiMODProLinkLORAWAN_RadioStackConfig::Retransmissions

max number of retransmissions (for C-Data) to use

## ◆ SubBandMask1

UINT8 TWiMODProLinkLORAWAN_RadioStackConfig::SubBandMask1

Sub-band selection for 125 kHz bandwidth channels

## ◆ SubBandMask2

UINT8 TWiMODProLinkLORAWAN_RadioStackConfig::SubBandMask2

Sub-band selection for 500 kHz bandwidth channels

## ◆ TXPowerLevel

UINT8 TWiMODProLinkLORAWAN_RadioStackConfig::TXPowerLevel

default / initial power level settings to be used

## ◆ WrongParamErrCode

UINT8 TWiMODProLinkLORAWAN_RadioStackConfig::WrongParamErrCode

error code in case of a wrong parameter (

See also
  LORAWAN_STK_PARAM_ERR defines)

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_ProLink_IDs.h