| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Typedefs | Enumerations
WiMOD_SAP_LORAWAN_IDs_AS923.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Typedefs
typedef enum TLoRaWANDataRateAS923 | TLoRaWANDataRateAS923
| LoRa data rate definitions for Asia 923 MHz Band. More...
typedef enum TLoRaWAN_Channel_AS_1 | TLoRaWAN_Channel_AS_1
| ‍** More...
typedef enum TLoRaWAN_Channel_AS_2 | TLoRaWAN_Channel_AS_2
| Channel definition for AS 923MHz Band 2.
typedef enum TLoRaWAN_Channel_AS_3 | TLoRaWAN_Channel_AS_3
| Channel definition for AS 923MHz Band 3.

## Enumerations
enum | TLoRaWANDataRateAS923 { LoRaWAN_DataRate_AS923_LoRa_SF12_125kHz = 0, LoRaWAN_DataRate_AS923_LoRa_SF11_125kHz, LoRaWAN_DataRate_AS923_LoRa_SF10_125kHz, LoRaWAN_DataRate_AS923_LoRa_SF9_125kHz, LoRaWAN_DataRate_AS923_LoRa_SF8_125kHz, LoRaWAN_DataRate_AS923_LoRa_SF7_125kHz, LoRaWAN_DataRate_AS923_LoRa_SF7_250kHz, LoRaWAN_DataRate_AS923_LoRa_FSK }
| LoRa data rate definitions for Asia 923 MHz Band. More...
enum | TLoRaWAN_Channel_AS_1 { LoRaWAN_Channel_AS_923_2_Mhz = 0, LoRaWAN_Channel_AS_923_4_Mhz = 1, LoRaWAN_Channel_AS_923_2_Mhz_2 = 128 }
| ‍** More...
enum | TLoRaWAN_Channel_AS_2 { LoRaWAN_Channel_AS_921_4_Mhz = 0, LoRaWAN_Channel_AS_921_6_Mhz = 1, LoRaWAN_Channel_AS_921_4_Mhz_2 = 128 }
| Channel definition for AS 923MHz Band 2. More...
enum | TLoRaWAN_Channel_AS_3 { LoRaWAN_Channel_AS_916_6_Mhz = 0, LoRaWAN_Channel_AS_916_8_Mhz = 1, LoRaWAN_Channel_AS_916_6_Mhz_2 = 128 }
| Channel definition for AS 923MHz Band 3. More...

## Typedef Documentation

## ◆ TLoRaWAN_Channel_AS_1

typedef enum TLoRaWAN_Channel_AS_1 TLoRaWAN_Channel_AS_1

‍**

‍**

Channel definition for AS 923MHz Band 1

## ◆ TLoRaWANDataRateAS923

typedef enum TLoRaWANDataRateAS923 TLoRaWANDataRateAS923

LoRa data rate definitions for Asia 923 MHz Band.

Version
  0.1

## Enumeration Type Documentation

## ◆ TLoRaWAN_Channel_AS_1

enum TLoRaWAN_Channel_AS_1

‍**

‍**

Channel definition for AS 923MHz Band 1

Enumerator
LoRaWAN_Channel_AS_923_2_Mhz | carrier frequency of 923.200 MHz
LoRaWAN_Channel_AS_923_4_Mhz | carrier frequency of 923.400 MHz
LoRaWAN_Channel_AS_923_2_Mhz_2 | carrier frequency of 923.200 MHz

## ◆ TLoRaWAN_Channel_AS_2

enum TLoRaWAN_Channel_AS_2

Channel definition for AS 923MHz Band 2.

Enumerator
LoRaWAN_Channel_AS_921_4_Mhz | carrier frequency of 921.400 MHz
LoRaWAN_Channel_AS_921_6_Mhz | carrier frequency of 921.600 MHz
LoRaWAN_Channel_AS_921_4_Mhz_2 | carrier frequency of 921.400 MHz

## ◆ TLoRaWAN_Channel_AS_3

enum TLoRaWAN_Channel_AS_3

Channel definition for AS 923MHz Band 3.

Enumerator
LoRaWAN_Channel_AS_916_6_Mhz | carrier frequency of 916.600 MHz
LoRaWAN_Channel_AS_916_8_Mhz | carrier frequency of 916.800 MHz
LoRaWAN_Channel_AS_916_6_Mhz_2 | carrier frequency of 916.600 MHz

## ◆ TLoRaWANDataRateAS923

enum TLoRaWANDataRateAS923

LoRa data rate definitions for Asia 923 MHz Band.

Version
  0.1

Enumerator
LoRaWAN_DataRate_AS923_LoRa_SF12_125kHz | LoRa Spreading factor 12 using 125kHz bandwidth
LoRaWAN_DataRate_AS923_LoRa_SF11_125kHz | LoRa Spreading factor 11 using 125kHz bandwidth
LoRaWAN_DataRate_AS923_LoRa_SF10_125kHz | LoRa Spreading factor 10 using 125kHz bandwidth
LoRaWAN_DataRate_AS923_LoRa_SF9_125kHz | LoRa Spreading factor 9 using 125kHz bandwidth
LoRaWAN_DataRate_AS923_LoRa_SF8_125kHz | LoRa Spreading factor 8 using 125kHz bandwidth
LoRaWAN_DataRate_AS923_LoRa_SF7_125kHz | LoRa Spreading factor 7 using 125kHz bandwidth
LoRaWAN_DataRate_AS923_LoRa_SF7_250kHz | LoRa Spreading factor 7 using 250kHz bandwidth
LoRaWAN_DataRate_AS923_LoRa_FSK | FSK modulation; LoRa settings not applicable