| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLR_RLT_Parameter Struct Reference

Structure containing a general RadioLink HCI message. More...

`#include <SAP/WiMOD_SAP_RLT_IDs.h>`

## Public Attributes
UINT8 | DestGroupAddress
UINT16 | DestDevAddress
UINT8 | PacketSize
UINT16 | NumPackets
TRLT_TestMode | TestMode

## Detailed Description

Structure containing a general RadioLink HCI message.

## Member Data Documentation

## ◆ DestDevAddress

UINT16 TWiMODLR_RLT_Parameter::DestDevAddress

address of peer device

## ◆ DestGroupAddress

UINT8 TWiMODLR_RLT_Parameter::DestGroupAddress

destionation group of peer device

## ◆ NumPackets

UINT16 TWiMODLR_RLT_Parameter::NumPackets

number of tests / test transmisions

## ◆ PacketSize

UINT8 TWiMODLR_RLT_Parameter::PacketSize

number of dummy payload bytes to use

## ◆ TestMode

TRLT_TestMode TWiMODLR_RLT_Parameter::TestMode

test mode to use;

See also
  TRLT_TestMode

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_RLT_IDs.h