| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

WiMOD_SAP_LoRaWAN Member List

This is the complete list of members for WiMOD_SAP_LoRaWAN, including all inherited members.

ActivateDevice(TWiMODLORAWAN_ActivateDeviceData &activationData, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_Data *loraWanRxData) | WiMOD_SAP_LoRaWAN |
convert(TWiMODLR_HCIMessage &rxMsg, TWiMODLORAWAN_TxIndData *sendIndData) | WiMOD_SAP_LoRaWAN |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_MacCmdData *loraWanMacCmdData) | WiMOD_SAP_LoRaWAN |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_JoinedNwkData *joinedNwkData) | WiMOD_SAP_LoRaWAN |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_ACK_Data *ackData) | WiMOD_SAP_LoRaWAN |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_NoData_Data *info) | WiMOD_SAP_LoRaWAN |
DeactivateDevice(UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
DispatchLoRaWANMessage(TWiMODLR_HCIMessage &rxMsg) (defined in WiMOD_SAP_LoRaWAN) | WiMOD_SAP_LoRaWAN | virtual
FactoryReset(UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetCustomConfig(INT8 *rfGain, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetDeviceEUI(UINT8 *deviceEUI, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetNwkStatus(TWiMODLORAWAN_NwkStatus_Data *nwkStatus, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetRadioStackConfig(TWiMODLORAWAN_RadioStackConfig *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetSupportedBands(TWiMODLORAWAN_SupportedBands *supportedBands, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetTxPowerLimitConfig(TWiMODLORAWAN_TxPwrLimitConfig *txPwrLimitCfg, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
JoinNetwork(UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
ReactivateDevice(UINT32 *devAdr, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
RegisterDeviceTimeAnsIndicationClient(TNwkDeviceTimeAnsIndicationCallback cb) | WiMOD_SAP_LoRaWAN | virtual
RegisterJoinedNwkIndicationClient(TJoinedNwkIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterJoinTxIndicationClient(TJoinTxIndicationCallback cb) | WiMOD_SAP_LoRaWAN | virtual
RegisterLinkDisconnectIndicationClient(TLinkDisconnectIndicationCallback cb) | WiMOD_SAP_LoRaWAN | virtual
RegisterNoDataIndicationClient(TNoDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterResetDevNonceIndicationClient(TResetDevNonceIndicationCallback cb) | WiMOD_SAP_LoRaWAN | virtual
RegisterRxAckIndicationClient(TRxAckIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterRxCDataIndicationClient(TRxCDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterRxMacCmdIndicationClient(TRxMacCmdIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterRxUDataIndicationClient(TRxUDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterTxCDataIndicationClient(TTxCDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterTxUDataIndicationClient(TTxUDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
SendCData(const TWiMODLORAWAN_TX_Data *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SendMacCmd(const TWiMODLORAWAN_MacCmd *cmd, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SendUData(const TWiMODLORAWAN_TX_Data *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetBatteryLevelStatus(UINT8 battStatus, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetCustomConfig(const INT8 rfGain, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetDeviceEUI(const UINT8 *deviceEUI, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetJoinParameter(TWiMODLORAWAN_JoinParams &joinParams, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetRadioStackConfig(TWiMODLORAWAN_RadioStackConfig *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
setRegion(TLoRaWANregion regionalSetting) | WiMOD_SAP_LoRaWAN | virtual
SetTxPowerLimitConfig(TWiMODLORAWAN_TxPwrLimitConfig &txPwrLimitCfg, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
WiMOD_SAP_LoRaWAN(TWiMODLRHCI *hci, UINT8 *buffer, UINT16 bufferSize) | WiMOD_SAP_LoRaWAN |
~WiMOD_SAP_LoRaWAN(void) | WiMOD_SAP_LoRaWAN | virtual