| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

WiMODGlobalLink24 Member List

This is the complete list of members for WiMODGlobalLink24, including all inherited members.

ActivateDevice(TWiMODGlobalLink24_ActivateDeviceData &activationData, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
begin(TLoRaWANregion region=LoRaWAN_Region_proprietary_WW2G4) | WiMODGlobalLink24 |
ClearRtcAlarm(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
ConnectViaOTAA(const uint8_t *appEUI=NULL, const uint8_t *appKey=NULL) | WiMODGlobalLink24 |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODGlobalLink24_RX_Data *globalLink24RxData) | WiMODGlobalLink24 |
convert(TWiMODLR_HCIMessage &rxMsg, TWiMODGlobalLink24_TxIndData *sendIndData) | WiMODGlobalLink24 |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODGlobalLink24_RX_MacCmdData *globalLink24MacCmdData) | WiMODGlobalLink24 |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODGlobalLink24_RX_JoinedNwkData *joinedNwkData) | WiMODGlobalLink24 |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODGlobalLink24_RX_ACK_Data *ackData) | WiMODGlobalLink24 |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODGlobalLink24_NoData_Data *info) | WiMODGlobalLink24 |
ConvertAppEuiStrToArray(char *appEuiStr, uint8_t *appEuiArray) | WiMODGlobalLink24 |
ConvertAppKeyStrToArray(char *appKeyStr, uint8_t *appKeyArray) | WiMODGlobalLink24 |
ConvertAppSKeyStrToArray(char *appSKeyStr, uint8_t *appSKeyArray) | WiMODGlobalLink24 |
ConvertNwkSKeyStrToArray(char *nwkSKeyStr, uint8_t *nwkSKeyArray) | WiMODGlobalLink24 |
DeactivateDevice(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
EnableWakeupSequence(bool flag) (defined in WiMODGlobalLink24) | WiMODGlobalLink24 |
end(void) | WiMODGlobalLink24 |
ExecuteGenericCmd(TWiMODLR_Generic_CmdInfo *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
FactoryReset(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetCustomConfig(INT8 *rfGain, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetDeviceEUI(UINT8 *deviceEUI, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetDeviceInfo(TWiMODLR_DevMgmt_DevInfoLoRaWan *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetFirmwareInfo(TWiMODLR_DevMgmt_FwInfo *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetHciConfig(TWiMODLR_DevMgmt_HciConfig *hciConfig, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetLastHciResult(void) | WiMODGlobalLink24 |
GetLastResponseStatus(void) | WiMODGlobalLink24 |
GetNwkStatus(TWiMODGlobalLink24_NwkStatus_Data *nwkStatus, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetOperationMode(TWiMOD_OperationMode *opMode, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetRadioStackConfig(TWiMODGlobalLink24_RadioStackConfig *data, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetRtc(UINT32 *rtcTime, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetRtcAlarm(TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetSupportedBands(TWiMODGlobalLink24_SupportedBands *supportedBands, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GetSystemStatus(TWiMODLR_DevMgmt_SystemStatusLorawan *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
GlobalLinkImp (defined in WiMODGlobalLink24) | WiMODGlobalLink24 | protected
JoinNetwork(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
Ping(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
PrintBasicDeviceInfo(Stream &s) (defined in WiMODGlobalLink24) | WiMODGlobalLink24 |
Process(void) (defined in WiMODGlobalLink24) | WiMODGlobalLink24 |
ReactivateDevice(UINT32 *devAdr, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
RegisterJoinedNwkIndicationClient(TJoinedNwkIndicationCallback cb) | WiMODGlobalLink24 |
RegisterJoinTxIndicationClient(TJoinTxIndicationCallback cb) | WiMODGlobalLink24 |
RegisterNoDataIndicationClient(TNoDataIndicationCallback cb) | WiMODGlobalLink24 |
RegisterPowerUpIndicationClient(TDevMgmtPowerUpCallback cb) | WiMODGlobalLink24 |
RegisterRtcAlarmIndicationClient(TDevMgmtRtcAlarmCallback cb) | WiMODGlobalLink24 |
RegisterRxAckIndicationClient(TRxAckIndicationCallback cb) | WiMODGlobalLink24 |
RegisterRxCDataIndicationClient(TRxCDataIndicationCallback cb) | WiMODGlobalLink24 |
RegisterRxMacCmdIndicationClient(TRxMacCmdIndicationCallback cb) | WiMODGlobalLink24 |
RegisterRxUDataIndicationClient(TRxUDataIndicationCallback cb) | WiMODGlobalLink24 |
RegisterTxCDataIndicationClient(TTxCDataIndicationCallback cb) | WiMODGlobalLink24 |
RegisterTxUDataIndicationClient(TTxUDataIndicationCallback cb) | WiMODGlobalLink24 |
Reset(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SendCData(const TWiMODGlobalLink24_TX_Data *data, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SendMacCmd(const TWiMODGlobalLink24_MacCmd *cmd, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SendUData(const TWiMODGlobalLink24_TX_Data *data, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SetBatteryLevelStatus(UINT8 battStatus, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SetCustomConfig(const INT8 rfGain, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SetDeviceEUI(const UINT8 *deviceEUI, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SetHciConfig(TWiMODLR_DevMgmt_HciConfig &hciConfig, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SetJoinParameter(TWiMODGlobalLink24_JoinParams &joinParams, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SetOperationMode(const TWiMOD_OperationMode opMode, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SetRadioStackConfig(TWiMODGlobalLink24_RadioStackConfig *data, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SetRtc(const UINT32 rtcTime, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
SetRtcAlarm(const TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODGlobalLink24 |
WiMODGlobalLink24(Stream &s) | WiMODGlobalLink24 |
~WiMODGlobalLink24(void) | WiMODGlobalLink24 |