| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLR_HCIMessage Struct Reference

basic low level HCI message structure used for all serial messages to/from WiMOD More...

`#include <HCI/WiMODLRHCI.h>`

## Public Attributes
UINT16 | Length
UINT8 | SapID
UINT8 | MsgID
UINT8 | Payload [WIMODLR_HCI_MSG_PAYLOAD_SIZE]
UINT8 | CRC16 [WIMODLR_HCI_MSG_FCS_SIZE]

## Detailed Description

basic low level HCI message structure used for all serial messages to/from WiMOD

## Member Data Documentation

## ◆ CRC16

UINT8 TWiMODLR_HCIMessage::CRC16[WIMODLR_HCI_MSG_FCS_SIZE]

Frame Check Sum field; a 16-bit CRC algorithm is used

## ◆ Length

UINT16 TWiMODLR_HCIMessage::Length

length indicator; this field is not being transfered via serial link

## ◆ MsgID

UINT8 TWiMODLR_HCIMessage::MsgID

Command OpCode ID for this message

## ◆ Payload

UINT8 TWiMODLR_HCIMessage::Payload[WIMODLR_HCI_MSG_PAYLOAD_SIZE]

Payload field; content is command specific

## ◆ SapID

UINT8 TWiMODLR_HCIMessage::SapID

Service Access Point ID for this message

The documentation for this struct was generated from the following file:

- HCI/WiMODLRHCI.h