| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLORAWAN_TxPwrLimitConfig Struct Reference

data structure for TX Power Limits More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

## Public Attributes
UINT8 | NumOfEntries
UINT8 | SubBandIndex [(WiMODLORAWAN_APP_PAYLOAD_LEN/3)]
UINT8 | TxPwrLimitFlag [(WiMODLORAWAN_APP_PAYLOAD_LEN/3)]
UINT8 | TxPwrLimitValue [(WiMODLORAWAN_APP_PAYLOAD_LEN/3)]
UINT8 | WrongParamErrCode

## Detailed Description

data structure for TX Power Limits

## Member Data Documentation

## ◆ NumOfEntries

UINT8 TWiMODLORAWAN_TxPwrLimitConfig::NumOfEntries

number of entries in this data structure

## ◆ SubBandIndex

UINT8 TWiMODLORAWAN_TxPwrLimitConfig::SubBandIndex[(WiMODLORAWAN_APP_PAYLOAD_LEN/3)]

SubBandIndex

## ◆ TxPwrLimitFlag

UINT8 TWiMODLORAWAN_TxPwrLimitConfig::TxPwrLimitFlag[(WiMODLORAWAN_APP_PAYLOAD_LEN/3)]

TX Power Limit Flag

## ◆ TxPwrLimitValue

UINT8 TWiMODLORAWAN_TxPwrLimitConfig::TxPwrLimitValue[(WiMODLORAWAN_APP_PAYLOAD_LEN/3)]

TX Power Limit Value

## ◆ WrongParamErrCode

UINT8 TWiMODLORAWAN_TxPwrLimitConfig::WrongParamErrCode

Optional error code for set operation (

See also
  LORAWAN_TX_PWR_LIMIT_ERR defines)

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h