| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Typedefs | Enumerations
WiMOD_SAP_GlobalLink24_IDs_WW2G4.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Typedefs
typedef enum TGlobalLink24DataRateWW2G4 | TGlobalLink24DataRateWW2G4
| LoRa data rate definitions for WW 2G4 MHz Band. More...
typedef enum TGlobalLink24_Channel_WW2G4 | TLoRaWAN_Channel_WW2G4
| Channel definition for WW2G4.

## Enumerations
enum | TGlobalLink24DataRateWW2G4 { LoRaWAN_DataRate_WW2G4_LoRa_SF12_812kHz = 0, LoRaWAN_DataRate_WW2G4_LoRa_SF11_812kHz, LoRaWAN_DataRate_WW2G4_LoRa_SF10_812kHz, LoRaWAN_DataRate_WW2G4_LoRa_SF9_812kHz, LoRaWAN_DataRate_WW2G4_LoRa_SF8_812kHz, LoRaWAN_DataRate_WW2G4_LoRa_SF7_812kHz, LoRaWAN_DataRate_WW2G4_LoRa_SF6_812kHz, LoRaWAN_DataRate_WW2G4_LoRa_SF5_812kHz }
| LoRa data rate definitions for WW 2G4 MHz Band. More...
enum | TGlobalLink24_Channel_WW2G4 { GlobalLink24_Channel_WW_2403_Mhz = 0, GlobalLink24_Channel_WW_2425_Mhz = 1, GlobalLink24_Channel_WW_2479_Mhz = 2, GlobalLink24_Channel_WW_2423_Mhz = 128 }
| Channel definition for WW2G4. More...

## Typedef Documentation

## ◆ TGlobalLink24DataRateWW2G4

typedef enum TGlobalLink24DataRateWW2G4 TGlobalLink24DataRateWW2G4

LoRa data rate definitions for WW 2G4 MHz Band.

Version
  0.1

## Enumeration Type Documentation

## ◆ TGlobalLink24_Channel_WW2G4

enum TGlobalLink24_Channel_WW2G4

Channel definition for WW2G4.

Enumerator
GlobalLink24_Channel_WW_2403_Mhz | carrier frequency of 2403 MHz
GlobalLink24_Channel_WW_2425_Mhz | carrier frequency of 2425 MHz
GlobalLink24_Channel_WW_2479_Mhz | carrier frequency of 2479 MHz
GlobalLink24_Channel_WW_2423_Mhz | carrier frequency of 2423 MHz

## ◆ TGlobalLink24DataRateWW2G4

enum TGlobalLink24DataRateWW2G4

LoRa data rate definitions for WW 2G4 MHz Band.

Version
  0.1

Enumerator
LoRaWAN_DataRate_WW2G4_LoRa_SF12_812kHz | LoRa Spreading factor 12 using 812kHz bandwidth
LoRaWAN_DataRate_WW2G4_LoRa_SF11_812kHz | LoRa Spreading factor 11 using 812kHz bandwidth
LoRaWAN_DataRate_WW2G4_LoRa_SF10_812kHz | LoRa Spreading factor 10 using 812kHz bandwidth
LoRaWAN_DataRate_WW2G4_LoRa_SF9_812kHz | LoRa Spreading factor 9 using 812kHz bandwidth
LoRaWAN_DataRate_WW2G4_LoRa_SF8_812kHz | LoRa Spreading factor 8 using 812kHz bandwidth
LoRaWAN_DataRate_WW2G4_LoRa_SF7_812kHz | LoRa Spreading factor 7 using 812kHz bandwidth
LoRaWAN_DataRate_WW2G4_LoRa_SF6_812kHz | LoRa Spreading factor 6 using 812kHz bandwidth
LoRaWAN_DataRate_WW2G4_LoRa_SF5_812kHz | LoRa Spreading factor 5 using 812kHz bandwidth