| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

WiMOD_SAP_LoRaWAN_ProLink Member List

This is the complete list of members for WiMOD_SAP_LoRaWAN_ProLink, including all inherited members.

ActivateDevice(TWiMODLORAWAN_ActivateDeviceData &activationData, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_DevTimeAnsInfo *info) | WiMOD_SAP_LoRaWAN_ProLink |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_McastData *mcastData) | WiMOD_SAP_LoRaWAN_ProLink |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_McastNoData *mcastErrData) | WiMOD_SAP_LoRaWAN_ProLink |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_Data *loraWanRxData) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink | inline
convert(TWiMODLR_HCIMessage &rxMsg, TWiMODLORAWAN_TxIndData *sendIndData) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink | inline
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_MacCmdData *loraWanMacCmdData) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink | inline
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_JoinedNwkData *joinedNwkData) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink | inline
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_RX_ACK_Data *ackData) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink | inline
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLORAWAN_NoData_Data *info) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink | inline
DeactivateDevice(UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
DispatchLoRaWANMessage(TWiMODLR_HCIMessage &rxMsg) (defined in WiMOD_SAP_LoRaWAN) | WiMOD_SAP_LoRaWAN | virtual
DispatchProLinkLoRaWANMessage(TWiMODLR_HCIMessage &rxMsg) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink |
FactoryReset(UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetCustomConfig(INT8 *rfGain, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetDeviceEUI(UINT8 *deviceEUI, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetDeviceNonce(UINT16 *devNonce, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN_ProLink |
GetJoinNonce(UINT16 *joinNonce, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN_ProLink |
GetMulticastConfig(TWiMODLORAWAN_McastConfig *mcastCfg, UINT8 *statusRsp) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink |
GetNwkStatus(TWiMODLORAWAN_NwkStatus_Data *nwkStatus, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetRadioStackConfig(TWiMODProLinkLORAWAN_RadioStackConfig *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN_ProLink | virtual
WiMOD_SAP_LoRaWAN::GetRadioStackConfig(TWiMODLORAWAN_RadioStackConfig *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetSupportedBands(TWiMODLORAWAN_SupportedBands *supportedBands, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
GetTxPowerLimitConfig(TWiMODLORAWAN_TxPwrLimitConfig *txPwrLimitCfg, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
JoinNetwork(UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
ReactivateDevice(UINT32 *devAdr, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
RegisterDeviceTimeAnsIndicationClient(TNwkDeviceTimeAnsIndicationCallback cb) | WiMOD_SAP_LoRaWAN_ProLink | virtual
RegisterJoinedNwkIndicationClient(TJoinedNwkIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterJoinTxIndicationClient(TJoinTxIndicationCallback cb) | WiMOD_SAP_LoRaWAN | virtual
RegisterLinkDisconnectIndicationClient(TLinkDisconnectIndicationCallback cb) | WiMOD_SAP_LoRaWAN_ProLink | virtual
RegisterMulticastDataIndicationClient(TMCastDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN_ProLink |
RegisterMulticastInvalidDataIndicationClient(TMCastInvalidDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN_ProLink |
RegisterNoDataIndicationClient(TNoDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterResetDevNonceIndicationClient(TResetDevNonceIndicationCallback cb) | WiMOD_SAP_LoRaWAN_ProLink | virtual
RegisterRxAckIndicationClient(TRxAckIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterRxCDataIndicationClient(TRxCDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterRxMacCmdIndicationClient(TRxMacCmdIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterRxUDataIndicationClient(TRxUDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterTxCDataIndicationClient(TTxCDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RegisterTxUDataIndicationClient(TTxUDataIndicationCallback cb) | WiMOD_SAP_LoRaWAN |
RemoveMulticastConfig(const UINT8 mcastIndex, UINT8 *statusRsp) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink |
SendCData(TWiMODProLinkLORAWAN_TX_Data *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN_ProLink |
WiMOD_SAP_LoRaWAN::SendCData(const TWiMODLORAWAN_TX_Data *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SendMacCmd(const TWiMODLORAWAN_MacCmd *cmd, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SendNwkTimeRequest(TWiMODLORAWAN_DevTimeReqInfo *devTimeInfo, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN_ProLink |
SendUData(TWiMODProLinkLORAWAN_TX_Data *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN_ProLink |
WiMOD_SAP_LoRaWAN::SendUData(const TWiMODLORAWAN_TX_Data *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetBatteryLevelStatus(UINT8 battStatus, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetCustomConfig(const INT8 rfGain, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetDeviceEUI(const UINT8 *deviceEUI, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetDeviceNonce(const UINT16 devNonce, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN_ProLink |
SetJoinNonce(const UINT16 joinNonce, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN_ProLink |
SetJoinParameter(TWiMODLORAWAN_JoinParams &joinParams, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
SetMulticastConfig(TWiMODLORAWAN_McastConfig &mcastCfg, UINT8 *statusRsp) (defined in WiMOD_SAP_LoRaWAN_ProLink) | WiMOD_SAP_LoRaWAN_ProLink |
SetRadioStackConfig(TWiMODProLinkLORAWAN_RadioStackConfig *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN_ProLink | virtual
WiMOD_SAP_LoRaWAN::SetRadioStackConfig(TWiMODLORAWAN_RadioStackConfig *data, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
setRegion(TProLinkLoRaWANregion regionalSetting) | WiMOD_SAP_LoRaWAN_ProLink | virtual
WiMOD_SAP_LoRaWAN::setRegion(TLoRaWANregion regionalSetting) | WiMOD_SAP_LoRaWAN | virtual
SetTxPowerLimitConfig(TWiMODLORAWAN_TxPwrLimitConfig &txPwrLimitCfg, UINT8 *statusRsp) | WiMOD_SAP_LoRaWAN | virtual
WiMOD_SAP_LoRaWAN(TWiMODLRHCI *hci, UINT8 *buffer, UINT16 bufferSize) | WiMOD_SAP_LoRaWAN |
WiMOD_SAP_LoRaWAN_ProLink(TWiMODLRHCI *hci, UINT8 *buffer, UINT16 bufferSize) | WiMOD_SAP_LoRaWAN_ProLink |
~WiMOD_SAP_LoRaWAN(void) | WiMOD_SAP_LoRaWAN | virtual
~WiMOD_SAP_LoRaWAN_ProLink(void) | WiMOD_SAP_LoRaWAN_ProLink | virtual