| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Typedefs | Enumerations
WiMOD_SAP_LORAWAN_IDs_RU868.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Typedefs
typedef enum TLoRaWAN_Channel_RussiaOne | TLoRaWAN_Channel_RussiaOne
| LoRaWAN RUSSIA channel map ONE. More...
typedef enum TLoRaWAN_Channel_RussiaTwo | TLoRaWAN_Channel_RussiaTwo
| LoRaWAN RUSSIA channel map TWO.
typedef enum TLoRaWAN_Channel_RussiaThree | TLoRaWAN_Channel_RussiaThree
| LoRaWAN RUSSIA channel map THREE.
typedef enum TLoRaWAN_Channel_RussiaFour | TLoRaWAN_Channel_RussiaFour
| LoRaWAN RUSSIA channel map FOUR.
typedef enum TLoRaWAN_Channel_RussiaFive | TLoRaWAN_Channel_RussiaFive
| LoRaWAN RUSSIA channel map FIVE.
typedef enum TLoRaWAN_Channel_RussiaSix | TLoRaWAN_Channel_RussiaSix
| LoRaWAN RUSSIA channel map SIX.
typedef enum TLoRaWAN_Channel_RussiaSeven | TLoRaWAN_Channel_RussiaSeven
| LoRaWAN RUSSIA channel map SEVEN.
typedef enum TLoRaWANDataRateRU868 | TLoRaWANDataRateRU868
| LoRa data rate definitions for Russia 868 MHz Band.

## Enumerations
enum | TLoRaWAN_Channel_RussiaOne { LoRaWAN_Channel_Russia1_868_78_Mhz = 0, LoRaWAN_Channel_Russia1_868_95_Mhz = 1, LoRaWAN_Channel_Russia1_869_12_Mhz = 2, LoRaWAN_Channel_Russia1_864_1_Mhz = 3, LoRaWAN_Channel_Russia1_864_3_Mhz = 4, LoRaWAN_Channel_Russia1_864_5_Mhz = 5, LoRaWAN_Channel_Russia1_864_7_Mhz = 6, LoRaWAN_Channel_Russia1_864_9_Mhz = 128 }
| LoRaWAN RUSSIA channel map ONE. More...
enum | TLoRaWAN_Channel_RussiaTwo { LoRaWAN_Channel_Russia2_868_9_Mhz = 0, LoRaWAN_Channel_Russia2_868_7_Mhz = 1, LoRaWAN_Channel_Russia2_869_1_Mhz = 128 }
| LoRaWAN RUSSIA channel map TWO. More...
enum | TLoRaWAN_Channel_RussiaThree { LoRaWAN_Channel_Russia3_868_78_Mhz = 0, LoRaWAN_Channel_Russia3_868_95_Mhz = 1, LoRaWAN_Channel_Russia3_869_12_Mhz = 128 }
| LoRaWAN RUSSIA channel map THREE. More...
enum | TLoRaWAN_Channel_RussiaFour { LoRaWAN_Channel_Russia4_864_1_Mhz = 0, LoRaWAN_Channel_Russia4_864_3_Mhz = 1, LoRaWAN_Channel_Russia4_869_5_Mhz = 2, LoRaWAN_Channel_Russia4_864_64_Mhz = 3, LoRaWAN_Channel_Russia4_864_78_Mhz = 4, LoRaWAN_Channel_Russia4_868_78_Mhz = 5, LoRaWAN_Channel_Russia4_868_95_Mhz = 6, LoRaWAN_Channel_Russia4_869_12_Mhz = 7, LoRaWAN_Channel_Russia4_864_92_Mhz = 128 }
| LoRaWAN RUSSIA channel map FOUR. More...
enum | TLoRaWAN_Channel_RussiaFive { LoRaWAN_Channel_Russia5_864_5_Mhz = 0, LoRaWAN_Channel_Russia5_864_7_Mhz = 1, LoRaWAN_Channel_Russia5_864_9_Mhz = 2, LoRaWAN_Channel_Russia5_864_1_Mhz = 3, LoRaWAN_Channel_Russia5_864_3_Mhz = 4, LoRaWAN_Channel_Russia5_868_8_Mhz = 5, LoRaWAN_Channel_Russia5_869_05_Mhz = 128 }
| LoRaWAN RUSSIA channel map FIVE. More...
enum | TLoRaWAN_Channel_RussiaSix { LoRaWAN_Channel_Russia6_868_9_Mhz = 0, LoRaWAN_Channel_Russia6_869_1_Mhz = 1, LoRaWAN_Channel_Russia6_864_1_Mhz = 2, LoRaWAN_Channel_Russia6_864_3_Mhz = 3, LoRaWAN_Channel_Russia6_864_5_Mhz = 4, LoRaWAN_Channel_Russia6_864_7_Mhz = 5, LoRaWAN_Channel_Russia6_864_9_Mhz = 6, LoRaWAN_Channel_Russia6_869_1_Mhz_2 = 128 }
| LoRaWAN RUSSIA channel map SIX. More...
enum | TLoRaWAN_Channel_RussiaSeven { LoRaWAN_Channel_Russia7_868_9_Mhz = 0, LoRaWAN_Channel_Russia7_869_1_Mhz = 1, LoRaWAN_Channel_Russia7_869_1_Mhz_2 = 128 }
| LoRaWAN RUSSIA channel map SEVEN. More...
enum | TLoRaWANDataRateRU868 { LoRaWAN_DataRate_RU868_LoRa_SF12_125kHz = 0, LoRaWAN_DataRate_RU868_LoRa_SF11_125kHz, LoRaWAN_DataRate_RU868_LoRa_SF10_125kHz, LoRaWAN_DataRate_RU868_LoRa_SF9_125kHz, LoRaWAN_DataRate_RU868_LoRa_SF8_125kHz, LoRaWAN_DataRate_RU868_LoRa_SF7_125kHz, LoRaWAN_DataRate_RU868_LoRa_SF7_250kHz, LoRaWAN_DataRate_RU868_LoRa_FSK }
| LoRa data rate definitions for Russia 868 MHz Band. More...

## Typedef Documentation

## ◆ TLoRaWAN_Channel_RussiaOne

typedef enum TLoRaWAN_Channel_RussiaOne TLoRaWAN_Channel_RussiaOne

LoRaWAN RUSSIA channel map ONE.

Version
  0.1

## Enumeration Type Documentation

## ◆ TLoRaWAN_Channel_RussiaFive

enum TLoRaWAN_Channel_RussiaFive

LoRaWAN RUSSIA channel map FIVE.

Enumerator
LoRaWAN_Channel_Russia5_864_5_Mhz | carrier frequency of 864.500 MHz
LoRaWAN_Channel_Russia5_864_7_Mhz | carrier frequency of 864.700 MHz
LoRaWAN_Channel_Russia5_864_9_Mhz | carrier frequency of 864.800 MHz
LoRaWAN_Channel_Russia5_864_1_Mhz | carrier frequency of 864.100 MHz
LoRaWAN_Channel_Russia5_864_3_Mhz | carrier frequency of 864.300 MHz
LoRaWAN_Channel_Russia5_868_8_Mhz | carrier frequency of 868.800 MHz
LoRaWAN_Channel_Russia5_869_05_Mhz | carrier frequency of 869.050 MHz

## ◆ TLoRaWAN_Channel_RussiaFour

enum TLoRaWAN_Channel_RussiaFour

LoRaWAN RUSSIA channel map FOUR.

Enumerator
LoRaWAN_Channel_Russia4_864_1_Mhz | carrier frequency of 864.100 MHz
LoRaWAN_Channel_Russia4_864_3_Mhz | carrier frequency of 864.300 MHz
LoRaWAN_Channel_Russia4_869_5_Mhz | carrier frequency of 864.500 MHz
LoRaWAN_Channel_Russia4_864_64_Mhz | carrier frequency of 864.640 MHz
LoRaWAN_Channel_Russia4_864_78_Mhz | carrier frequency of 864.780 MHz
LoRaWAN_Channel_Russia4_868_78_Mhz | carrier frequency of 868.780 MHz
LoRaWAN_Channel_Russia4_868_95_Mhz | carrier frequency of 868.950 MHz
LoRaWAN_Channel_Russia4_869_12_Mhz | carrier frequency of 869.120 MHz
LoRaWAN_Channel_Russia4_864_92_Mhz | carrier frequency of 864.920 MHz

## ◆ TLoRaWAN_Channel_RussiaOne

enum TLoRaWAN_Channel_RussiaOne

LoRaWAN RUSSIA channel map ONE.

Version
  0.1

Enumerator
LoRaWAN_Channel_Russia1_868_78_Mhz | carrier frequency of 864.100 MHz
LoRaWAN_Channel_Russia1_868_95_Mhz | carrier frequency of 864.300 MHz
LoRaWAN_Channel_Russia1_869_12_Mhz | carrier frequency of 864.500 MHz
LoRaWAN_Channel_Russia1_864_1_Mhz | carrier frequency of 864.700 MHz
LoRaWAN_Channel_Russia1_864_3_Mhz | carrier frequency of 868.780 MHz
LoRaWAN_Channel_Russia1_864_5_Mhz | carrier frequency of 868.950 MHz
LoRaWAN_Channel_Russia1_864_7_Mhz | carrier frequency of 869.120 MHz
LoRaWAN_Channel_Russia1_864_9_Mhz | carrier frequency of 864.900 MHz

## ◆ TLoRaWAN_Channel_RussiaSeven

enum TLoRaWAN_Channel_RussiaSeven

LoRaWAN RUSSIA channel map SEVEN.

Enumerator
LoRaWAN_Channel_Russia7_868_9_Mhz | carrier frequency of 868.900 MHz
LoRaWAN_Channel_Russia7_869_1_Mhz | carrier frequency of 869.100 MHz
LoRaWAN_Channel_Russia7_869_1_Mhz_2 | carrier frequency of 869.100 MHz

## ◆ TLoRaWAN_Channel_RussiaSix

enum TLoRaWAN_Channel_RussiaSix

LoRaWAN RUSSIA channel map SIX.

Enumerator
LoRaWAN_Channel_Russia6_868_9_Mhz | carrier frequency of 868.900 MHz
LoRaWAN_Channel_Russia6_869_1_Mhz | carrier frequency of 869.100 MHz
LoRaWAN_Channel_Russia6_864_1_Mhz | carrier frequency of 864.100 MHz
LoRaWAN_Channel_Russia6_864_3_Mhz | carrier frequency of 864.300 MHz
LoRaWAN_Channel_Russia6_864_5_Mhz | carrier frequency of 864.500 MHz
LoRaWAN_Channel_Russia6_864_7_Mhz | carrier frequency of 864.700 MHz
LoRaWAN_Channel_Russia6_864_9_Mhz | carrier frequency of 864.900 MHz
LoRaWAN_Channel_Russia6_869_1_Mhz_2 | carrier frequency of 869.100 MHz

## ◆ TLoRaWAN_Channel_RussiaThree

enum TLoRaWAN_Channel_RussiaThree

LoRaWAN RUSSIA channel map THREE.

Enumerator
LoRaWAN_Channel_Russia3_868_78_Mhz | carrier frequency of 868.780 MHz
LoRaWAN_Channel_Russia3_868_95_Mhz | carrier frequency of 868.950 MHz
LoRaWAN_Channel_Russia3_869_12_Mhz | carrier frequency of 869.120 MHz

## ◆ TLoRaWAN_Channel_RussiaTwo

enum TLoRaWAN_Channel_RussiaTwo

LoRaWAN RUSSIA channel map TWO.

Enumerator
LoRaWAN_Channel_Russia2_868_9_Mhz | carrier frequency of 868.900 MHz
LoRaWAN_Channel_Russia2_868_7_Mhz | carrier frequency of 868.700 MHz
LoRaWAN_Channel_Russia2_869_1_Mhz | carrier frequency of 869.100 MHz

## ◆ TLoRaWANDataRateRU868

enum TLoRaWANDataRateRU868

LoRa data rate definitions for Russia 868 MHz Band.

Enumerator
LoRaWAN_DataRate_RU868_LoRa_SF12_125kHz | LoRa Spreading factor 12 using 125kHz bandwidth
LoRaWAN_DataRate_RU868_LoRa_SF11_125kHz | LoRa Spreading factor 11 using 125kHz bandwidth
LoRaWAN_DataRate_RU868_LoRa_SF10_125kHz | LoRa Spreading factor 10 using 125kHz bandwidth
LoRaWAN_DataRate_RU868_LoRa_SF9_125kHz | LoRa Spreading factor 9 using 125kHz bandwidth
LoRaWAN_DataRate_RU868_LoRa_SF8_125kHz | LoRa Spreading factor 8 using 125kHz bandwidth
LoRaWAN_DataRate_RU868_LoRa_SF7_125kHz | LoRa Spreading factor 7 using 125kHz bandwidth
LoRaWAN_DataRate_RU868_LoRa_SF7_250kHz | LoRa Spreading factor 7 using 250kHz bandwidth
LoRaWAN_DataRate_RU868_LoRa_FSK | FSK modulation; LoRa settings not applicable