| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Member Functions | List of all members
WiMOD_SAP_Generic Class Reference

Implementation for the ServiceAccessPoint DeviceManagement. More...

`#include <SAP/WiMOD_SAP_Generic.h>`

## Public Member Functions
| WiMOD_SAP_Generic (TWiMODLRHCI *hci, UINT8 *buffer, UINT16 bufferSize)
| Constructor. More...
| ~WiMOD_SAP_Generic (void)
| Destructor.
TWiMODLRResultCodes | ExecuteGenericCmd (TWiMODLR_Generic_CmdInfo *info, UINT8 *statusRsp)
| Reset Cmd - Do a reset / reboot of the WiMOD. More...

## Detailed Description

Implementation for the ServiceAccessPoint DeviceManagement.

## Constructor & Destructor Documentation

## ◆ WiMOD_SAP_Generic()

WiMOD_SAP_Generic::WiMOD_SAP_Generic | ( | TWiMODLRHCI * | hci,
|  | UINT8 * | buffer,
|  | UINT16 | bufferSize
| ) |  |

Constructor.

Parameters

  hci | Pointer to HCI processor object
  buffer | pointer to storage area for building tx frames; MUST BE VALID
  bufferSize | size of the buffer

## Member Function Documentation

## ◆ ExecuteGenericCmd()

TWiMODLRResultCodes WiMOD_SAP_Generic::ExecuteGenericCmd | ( | TWiMODLR_Generic_CmdInfo * | info,
|  | UINT8 * | statusRsp
| ) |  |

Reset Cmd - Do a reset / reboot of the WiMOD.

Parameters

  info | pointer to store the received information
  statusRsp | pointer to store status byte of response mesg from WiMOD

Return values

  WiMODLR_RESULT_OK | if command transmit to WiMOD was ok

The documentation for this class was generated from the following files:

- SAP/WiMOD_SAP_Generic.h
- SAP/WiMOD_SAP_Generic.cpp