<map id="WiMODLRBASE_PLUS" name="WiMODLRBASE_PLUS">
<area shape="rect" id="node1" title="Main class representing the interface to the WiMOD running the firmware WiMODLR&#45;BASE_PLUS." alt="" coords="589,157,751,184"/>
<area shape="rect" id="node2" href="$class_t_wi_m_o_d_l_r_h_c_i.html" title="Internal helper class for processing SLIP frames." alt="" coords="275,5,393,32"/>
<area shape="rect" id="node3" href="$class_t_com_slip_client.html" title="Class definition for enabling OO inheritance." alt="" coords="32,5,153,32"/>
<area shape="rect" id="node4" href="$class_wi_m_o_d___s_a_p___r_l_t.html" title="Implementation for the ServiceAccessPoint RadioLinkTest (LR&#45;Base firmware only)" alt="" coords="267,56,401,83"/>
<area shape="rect" id="node5" href="$class_wi_m_o_d___s_a_p___radio_link.html" title="Implementation for the ServiceAccessPoint RadioLink (LR&#45;Base firmware only)" alt="" coords="247,107,421,133"/>
<area shape="rect" id="node6" href="$class_wi_m_o_d___s_a_p___sensor_app.html" title="Implementation for the ServiceAccessPoint SensorApp (LR&#45;Base_PLUS firmware only)" alt="" coords="244,157,424,184"/>
<area shape="rect" id="node7" href="$class_wi_m_o_d___s_a_p___remote_ctrl.html" title="Implementation for the ServiceAccessPoint RadioLink (LR&#45;Base firmware only)" alt="" coords="241,208,427,235"/>
<area shape="rect" id="node8" href="$class_wi_m_o_d___s_a_p___generic.html" title="Implementation for the ServiceAccessPoint DeviceManagement." alt="" coords="253,259,415,285"/>
<area shape="rect" id="node9" href="$class_wi_m_o_d___s_a_p___dev_mgmt___plus.html" title="Implementation for the ServiceAccessPoint DeviceManagement." alt="" coords="229,309,439,336"/>
<area shape="rect" id="node10" href="$class_wi_m_o_d___s_a_p___dev_mgmt.html" title="Implementation for the ServiceAccessPoint DeviceManagement." alt="" coords="5,309,180,336"/>
</map>
