| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLORAWAN_NwkStatus_Data Struct Reference

Structure containing all data about LoRaWAN network status. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

Inheritance diagram for TWiMODLORAWAN_NwkStatus_Data:
[legend]

## Public Attributes
UINT8 | NetworkStatus
UINT32 | DeviceAddress
UINT8 | DataRateIndex
UINT8 | PowerLevel
UINT8 | MaxPayloadSize
UINT8 | NumMacTransmissions

## Detailed Description

Structure containing all data about LoRaWAN network status.

## Member Data Documentation

## ◆ DataRateIndex

UINT8 TWiMODLORAWAN_NwkStatus_Data::DataRateIndex

used data rate index (

See also
  TLoRaWANDataRate*)

## ◆ DeviceAddress

UINT32 TWiMODLORAWAN_NwkStatus_Data::DeviceAddress

32bit DeviceAddress of module in LoRa network

## ◆ MaxPayloadSize

UINT8 TWiMODLORAWAN_NwkStatus_Data::MaxPayloadSize

maximum number of bytes allowed in payload field

## ◆ NetworkStatus

UINT8 TWiMODLORAWAN_NwkStatus_Data::NetworkStatus

Current NetworkStatus (

See also
  TLoRaWAN_NwkStatus)

## ◆ NumMacTransmissions

UINT8 TWiMODLORAWAN_NwkStatus_Data::NumMacTransmissions

number of transmissions configured by the LNS

## ◆ PowerLevel

UINT8 TWiMODLORAWAN_NwkStatus_Data::PowerLevel

transmit power in dBm

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h