| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLORAWAN_RX_ACK_Data Struct Reference

Data structure for received Acknowledgment data. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

Inheritance diagram for TWiMODLORAWAN_RX_ACK_Data:
[legend]

## Public Attributes
UINT8 | StatusFormat
UINT8 | ChannelIndex
UINT8 | DataRateIndex
INT8 | RSSI
INT8 | SNR
UINT8 | RxSlot
bool | OptionalInfoAvaiable

## Detailed Description

Data structure for received Acknowledgment data.

## Member Data Documentation

## ◆ ChannelIndex

UINT8 TWiMODLORAWAN_RX_ACK_Data::ChannelIndex

used channel index (

See also
  TLoRaWAN_Channel_* definitions)

## ◆ DataRateIndex

UINT8 TWiMODLORAWAN_RX_ACK_Data::DataRateIndex

used data rate index (

See also
  TLoRaWANDataRate*)

## ◆ OptionalInfoAvaiable

bool TWiMODLORAWAN_RX_ACK_Data::OptionalInfoAvaiable

are the optional value fields available

## ◆ RSSI

INT8 TWiMODLORAWAN_RX_ACK_Data::RSSI

RSSI value for the received packet

## ◆ RxSlot

UINT8 TWiMODLORAWAN_RX_ACK_Data::RxSlot

number of the rx slot that contained the message

## ◆ SNR

INT8 TWiMODLORAWAN_RX_ACK_Data::SNR

SNR value for the received packet

## ◆ StatusFormat

UINT8 TWiMODLORAWAN_RX_ACK_Data::StatusFormat

Status/Format Field for this message

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h