| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Typedefs | Enumerations
WiMOD_SAP_LORAWAN_IDs_EU868.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Typedefs
typedef enum TLoRaWANDataRateEU868 | TLoRaWANDataRateEU868
| LoRa data rate definitions for EU 868 MHz Band. More...
typedef enum TLoRaWAN_Channel_EU | TLoRaWAN_Channel_EU
| Channel definition for EU 868MHz Band.

## Enumerations
enum | TLoRaWANDataRateEU868 { LoRaWAN_DataRate_EU868_LoRa_SF12_125kHz = 0, LoRaWAN_DataRate_EU868_LoRa_SF11_125kHz, LoRaWAN_DataRate_EU868_LoRa_SF10_125kHz, LoRaWAN_DataRate_EU868_LoRa_SF9_125kHz, LoRaWAN_DataRate_EU868_LoRa_SF8_125kHz, LoRaWAN_DataRate_EU868_LoRa_SF7_125kHz, LoRaWAN_DataRate_EU868_LoRa_SF7_250kHz, LoRaWAN_DataRate_EU868_LoRa_FSK }
| LoRa data rate definitions for EU 868 MHz Band. More...
enum | TLoRaWAN_Channel_EU { LoRaWAN_Channel_EU_868_1_Mhz = 0, LoRaWAN_Channel_EU_868_3_Mhz = 1, LoRaWAN_Channel_EU_868_5_Mhz = 2, LoRaWAN_Channel_EU_869_525_Mhz = 128 }
| Channel definition for EU 868MHz Band. More...

## Typedef Documentation

## ◆ TLoRaWANDataRateEU868

typedef enum TLoRaWANDataRateEU868 TLoRaWANDataRateEU868

LoRa data rate definitions for EU 868 MHz Band.

Version
  0.1

## Enumeration Type Documentation

## ◆ TLoRaWAN_Channel_EU

enum TLoRaWAN_Channel_EU

Channel definition for EU 868MHz Band.

Enumerator
LoRaWAN_Channel_EU_868_1_Mhz | carrier frequency of 868.100 MHz
LoRaWAN_Channel_EU_868_3_Mhz | carrier frequency of 868.300 MHz
LoRaWAN_Channel_EU_868_5_Mhz | carrier frequency of 868.500 MHz
LoRaWAN_Channel_EU_869_525_Mhz | carrier frequency of 869.525 MHz

## ◆ TLoRaWANDataRateEU868

enum TLoRaWANDataRateEU868

LoRa data rate definitions for EU 868 MHz Band.

Version
  0.1

Enumerator
LoRaWAN_DataRate_EU868_LoRa_SF12_125kHz | LoRa Spreading factor 12 using 125kHz bandwidth
LoRaWAN_DataRate_EU868_LoRa_SF11_125kHz | LoRa Spreading factor 11 using 125kHz bandwidth
LoRaWAN_DataRate_EU868_LoRa_SF10_125kHz | LoRa Spreading factor 10 using 125kHz bandwidth
LoRaWAN_DataRate_EU868_LoRa_SF9_125kHz | LoRa Spreading factor 9 using 125kHz bandwidth
LoRaWAN_DataRate_EU868_LoRa_SF8_125kHz | LoRa Spreading factor 8 using 125kHz bandwidth
LoRaWAN_DataRate_EU868_LoRa_SF7_125kHz | LoRa Spreading factor 7 using 125kHz bandwidth
LoRaWAN_DataRate_EU868_LoRa_SF7_250kHz | LoRa Spreading factor 7 using 250kHz bandwidth
LoRaWAN_DataRate_EU868_LoRa_FSK | FSK modulation; LoRa settings not applicable