| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLORAWAN_McastNoData Struct Reference

Structure containing a MultiCast Data. More...

`#include <SAP/WiMOD_SAP_LORAWAN_ProLink_IDs.h>`

## Public Attributes
UINT8 | StatusFormat
UINT8 | ErrorCode
UINT32 | DeviceAddress

## Detailed Description

Structure containing a MultiCast Data.

## Member Data Documentation

## ◆ DeviceAddress

UINT32 TWiMODLORAWAN_McastNoData::DeviceAddress

address of the WiMOD within the Multicast context of LoRaWAN network

## ◆ ErrorCode

UINT8 TWiMODLORAWAN_McastNoData::ErrorCode

ErrorCode bit field

See also
  PROLINK_MCAST_ERR_* defines

## ◆ StatusFormat

UINT8 TWiMODLORAWAN_McastNoData::StatusFormat

Status/Format Field set by WiMOD;

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_ProLink_IDs.h