| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLR_DevMgmt_HciConfig Struct Reference

HCI Configuration Parameters. More...

`#include <SAP/WiMOD_SAP_DEVMGMT_IDs.h>`

## Public Attributes
UINT8 | StoreNwmFlag
UINT8 | Status
TWiMOD_HCI_Baudrate | BaudrateID
UINT16 | NumWakeUpChars
UINT8 | TxHoldTime
UINT8 | RxHoldTime

## Detailed Description

HCI Configuration Parameters.

## Member Data Documentation

## ◆ BaudrateID

TWiMOD_HCI_Baudrate TWiMODLR_DevMgmt_HciConfig::BaudrateID

Baudrate setting; see documentation

## ◆ NumWakeUpChars

UINT16 TWiMODLR_DevMgmt_HciConfig::NumWakeUpChars

Number of wakeUp chars; see documentation

## ◆ RxHoldTime

UINT8 TWiMODLR_DevMgmt_HciConfig::RxHoldTime

Rx hold time in ms; see documentation

## ◆ Status

UINT8 TWiMODLR_DevMgmt_HciConfig::Status

status flag; indicates if other values are vaild

## ◆ StoreNwmFlag

UINT8 TWiMODLR_DevMgmt_HciConfig::StoreNwmFlag

Store the config in NVM or RAM; 1 = store in NVM

## ◆ TxHoldTime

UINT8 TWiMODLR_DevMgmt_HciConfig::TxHoldTime

Tx hold time in ms; see documentation

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_DEVMGMT_IDs.h