| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Public Attributes | List of all members
TWiMODLORAWAN_RX_MacCmdData Struct Reference

Structure containing a received MAC command. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

Inheritance diagram for TWiMODLORAWAN_RX_MacCmdData:
[legend]

## Public Attributes
UINT8 | Length
UINT8 | MacCmdData [WiMODLORAWAN_APP_PAYLOAD_LEN]
UINT8 | ChannelIndex
UINT8 | DataRateIndex
INT8 | RSSI
INT8 | SNR
UINT8 | RxSlot
bool | OptionalInfoAvaiable

## Detailed Description

Structure containing a received MAC command.

## Member Data Documentation

## ◆ ChannelIndex

UINT8 TWiMODLORAWAN_RX_MacCmdData::ChannelIndex

used channel index (

See also
  TLoRaWAN_Channel_* definitions)

## ◆ DataRateIndex

UINT8 TWiMODLORAWAN_RX_MacCmdData::DataRateIndex

used data rate index (

See also
  TLoRaWANDataRate*)

## ◆ Length

UINT8 TWiMODLORAWAN_RX_MacCmdData::Length

length of the MAC command / data

## ◆ MacCmdData

UINT8 TWiMODLORAWAN_RX_MacCmdData::MacCmdData[WiMODLORAWAN_APP_PAYLOAD_LEN]

MAC command / data

## ◆ OptionalInfoAvaiable

bool TWiMODLORAWAN_RX_MacCmdData::OptionalInfoAvaiable

are the optional value fields available

## ◆ RSSI

INT8 TWiMODLORAWAN_RX_MacCmdData::RSSI

RSSI value for the received packet

## ◆ RxSlot

UINT8 TWiMODLORAWAN_RX_MacCmdData::RxSlot

number of the rx slot that contained the message

## ◆ SNR

INT8 TWiMODLORAWAN_RX_MacCmdData::SNR

SNR value for the received packet

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h