| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

WiMODLRBASE_PLUS Member List

This is the complete list of members for WiMODLRBASE_PLUS, including all inherited members.

begin(void) | WiMODLRBASE_PLUS | virtual
calcFreqToRegister(uint32_t freq, uint8_t *msb, uint8_t *mid, uint8_t *lsb) | WiMODLRBASE_PLUS |
calcRegisterToFreq(uint8_t msb, uint8_t mid, uint8_t lsb) | WiMODLRBASE_PLUS |
ClearRtcAlarm(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_RadioLink_Msg *radioLinkMsg) | WiMODLRBASE_PLUS |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_RadioLink_CdataInd *cDataTxInfo) | WiMODLRBASE_PLUS |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_RadioLink_UdataInd *cDataTxInfo) | WiMODLRBASE_PLUS |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_AckTxInd_Msg *txAckIndInfo) | WiMODLRBASE_PLUS |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_RLT_Status *statusData) | WiMODLRBASE_PLUS |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_SensorApp_SensorData *sensorData) | WiMODLRBASE_PLUS |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_SensorApp_AckSensorData *sensorAckData) | WiMODLRBASE_PLUS |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_RemoteCtrl_BtnPressed *btnInfo) | WiMODLRBASE_PLUS |
copyResultInfos(TWiMODLRResultCodes *hciResult, UINT8 *rspStatus, UINT8 successValue) (defined in WiMODLRBASE_PLUS) | WiMODLRBASE_PLUS | protected
EnableWakeupSequence(bool flag) (defined in TWiMODLRHCI) | TWiMODLRHCI |
end(void) | WiMODLRBASE_PLUS | virtual
ExecuteGenericCmd(TWiMODLR_Generic_CmdInfo *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetAesKey(UINT8 *key, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetDeviceInfo(TWiMODLR_DevMgmt_DevInfo *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetFirmwareInfo(TWiMODLR_DevMgmt_FwInfo *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetHciConfig(TWiMODLR_DevMgmt_HciConfig *hciConfig, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetLastHciResult(void) | WiMODLRBASE_PLUS |
GetLastResponseStatus(void) | WiMODLRBASE_PLUS |
GetOperationMode(TWiMOD_OperationMode *opMode, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetRadioConfig(TWiMODLR_DevMgmt_RadioConfigPlus *radioCfg, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetRtc(UINT32 *rtcTime, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetRtcAlarm(TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetRxMessage(void) (defined in TWiMODLRHCI) | TWiMODLRHCI |
GetSensorAppConfig(TWiMODLR_SensorApp_Config *config, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
GetSystemStatus(TWiMODLR_DevMgmt_SystemStatusPlus *info, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
Ping(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
PostMessage(UINT8 sapID, UINT8 msgID, UINT8 *payload, UINT16 length) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
Process(void) | TWiMODLRHCI |
ProcessRxMessage(UINT8 *rxBuffer, UINT16 length) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
ProcessUnexpectedRxMessage(TWiMODLR_HCIMessage &rxMsg) (defined in WiMODLRBASE_PLUS) | WiMODLRBASE_PLUS | protected virtual
RegisterAckRxClient(TRadioLinkAckRxIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterAckRxTimeoutClient(TRadioLinkAckRxTimeoutIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterAckTxCallback(TRadioLinkAckTxIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterBtnPressedClient(TRemoteCtrlBtnPressedIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterCDataRxClient(TRadioLinkCDataRxIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterCDataTxClient(TRadioLinkCDataTxIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterPowerUpIndicationClient(TDevMgmtPowerUpCallback cb) | WiMODLRBASE_PLUS |
RegisterRawDataRxClient(TRadioLinkRawDataRxIndicationCallback cb) (defined in WiMODLRBASE_PLUS) | WiMODLRBASE_PLUS |
RegisterRltStatusClient(TRltStatusIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterRtcAlarmIndicationClient(TDevMgmtRtcAlarmCallback cb) | WiMODLRBASE_PLUS |
RegisterSensorAppAckIndClient(TSensorAppAckIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterSensorAppDataIndClient(TSensorAppSensorDataIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterStackErrorClient(TWiMODStackErrorClient cb) (defined in TWiMODLRHCI) | TWiMODLRHCI |
RegisterUDataRxClient(TRadioLinkUDataRxIndicationCallback cb) | WiMODLRBASE_PLUS |
RegisterUDataTxClient(TRadioLinkUDataTxIndicationCallback cb) | WiMODLRBASE_PLUS |
Reset(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
ResetRadioConfig(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SapDevMgmt | WiMODLRBASE_PLUS | protected
SapGeneric | WiMODLRBASE_PLUS | protected
SapRadioLink | WiMODLRBASE_PLUS | protected
SapRemoteCtrl | WiMODLRBASE_PLUS | protected
SapRLT | WiMODLRBASE_PLUS | protected
SapSensor | WiMODLRBASE_PLUS | protected
SendCData(const TWiMODLR_RadioLink_Msg *txMsg, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SendHCIMessage(UINT8 dstSapID, UINT8 msgID, UINT8 rxMsgID, UINT8 *payload, UINT16 length) | TWiMODLRHCI |
SendHCIMessageWithoutRx(UINT8 dstSapID, UINT8 msgID, UINT8 *payload, UINT16 length) | TWiMODLRHCI |
SendPacket(UINT8 *txData, UINT16 length) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
SendUData(const TWiMODLR_RadioLink_Msg *txMsg, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SendWakeUpSequence(void) | TWiMODLRHCI |
SetAckData(const TWiMODLR_RadioLink_Msg *txMsg, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SetAesKey(const UINT8 *key, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SetHciConfig(TWiMODLR_DevMgmt_HciConfig &hciConfig, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SetOperationMode(const TWiMOD_OperationMode opMode, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SetRadioConfig(const TWiMODLR_DevMgmt_RadioConfigPlus *radioCfg, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SetRadioMode(const TRadioCfg_RadioMode radioMode, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SetRtc(const UINT32 rtcTime, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SetRtcAlarm(const TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
SetSensorAppConfig(const TWiMODLR_SensorApp_Config *config, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
StartRadioLinkTest(const TWiMODLR_RLT_Parameter *params, TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
StopRadioLinkTest(TWiMODLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE_PLUS |
TComSlipClient() (defined in TComSlipClient) | TComSlipClient | inline
TWiMODLRHCI(Stream &s) | TWiMODLRHCI |
WaitForResponse(UINT8 rxSapID, UINT8 rxMsgID) (defined in TWiMODLRHCI) | TWiMODLRHCI | protected
WiMODLRBASE_PLUS(Stream &s) | WiMODLRBASE_PLUS |
~TComSlipClient() (defined in TComSlipClient) | TComSlipClient | inline virtual
~TWiMODLRHCI(void) | TWiMODLRHCI |
~WiMODLRBASE_PLUS(void) | WiMODLRBASE_PLUS |