| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Typedefs | Enumerations
WiMOD_SAP_LORAWAN_IDs_IL915.h File Reference
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Typedefs
typedef enum TLoRaWANDataRateIL915 | TLoRaWANDataRateIL915
| LoRa data rate definitions for Israel 915 MHz Band. More...
typedef enum TLoRaWAN_Channel_IL | TLoRaWAN_Channel_IL
| Channel definition for IL 915MHz Band.

## Enumerations
enum | TLoRaWANDataRateIL915 { LoRaWAN_DataRate_IL915_LoRa_SF12_125kHz = 0, LoRaWAN_DataRate_IL915_LoRa_SF11_125kHz, LoRaWAN_DataRate_IL915_LoRa_SF10_125kHz, LoRaWAN_DataRate_IL915_LoRa_SF9_125kHz, LoRaWAN_DataRate_IL915_LoRa_SF8_125kHz, LoRaWAN_DataRate_IL915_LoRa_SF7_125kHz, LoRaWAN_DataRate_IL915_LoRa_SF7_250kHz, LoRaWAN_DataRate_IL915_LoRa_FSK }
| LoRa data rate definitions for Israel 915 MHz Band. More...
enum | TLoRaWAN_Channel_IL { LoRaWAN_Channel_IL_915_7_Mhz = 0, LoRaWAN_Channel_IL_915_9_Mhz = 1, LoRaWAN_Channel_IL_916_1_Mhz = 2, LoRaWAN_Channel_IL_916_3_Mhz = 128 }
| Channel definition for IL 915MHz Band. More...

## Typedef Documentation

## ◆ TLoRaWANDataRateIL915

typedef enum TLoRaWANDataRateIL915 TLoRaWANDataRateIL915

LoRa data rate definitions for Israel 915 MHz Band.

Version
  0.1

## Enumeration Type Documentation

## ◆ TLoRaWAN_Channel_IL

enum TLoRaWAN_Channel_IL

Channel definition for IL 915MHz Band.

Enumerator
LoRaWAN_Channel_IL_915_7_Mhz | carrier frequency of 915.700 MHz
LoRaWAN_Channel_IL_915_9_Mhz | carrier frequency of 915.900 MHz
LoRaWAN_Channel_IL_916_1_Mhz | carrier frequency of 916.100 MHz
LoRaWAN_Channel_IL_916_3_Mhz | carrier frequency of 916.300 MHz

## ◆ TLoRaWANDataRateIL915

enum TLoRaWANDataRateIL915

LoRa data rate definitions for Israel 915 MHz Band.

Version
  0.1

Enumerator
LoRaWAN_DataRate_IL915_LoRa_SF12_125kHz | LoRa Spreading factor 12 using 125kHz bandwidth
LoRaWAN_DataRate_IL915_LoRa_SF11_125kHz | LoRa Spreading factor 11 using 125kHz bandwidth
LoRaWAN_DataRate_IL915_LoRa_SF10_125kHz | LoRa Spreading factor 10 using 125kHz bandwidth
LoRaWAN_DataRate_IL915_LoRa_SF9_125kHz | LoRa Spreading factor 9 using 125kHz bandwidth
LoRaWAN_DataRate_IL915_LoRa_SF8_125kHz | LoRa Spreading factor 8 using 125kHz bandwidth
LoRaWAN_DataRate_IL915_LoRa_SF7_125kHz | LoRa Spreading factor 7 using 125kHz bandwidth
LoRaWAN_DataRate_IL915_LoRa_SF7_250kHz | LoRa Spreading factor 7 using 250kHz bandwidth
LoRaWAN_DataRate_IL915_LoRa_FSK | FSK modulation; LoRa settings not applicable