| Demo HCI Implementation for WiMOD-LR Devices V2.0.3

Classes | Typedefs | Enumerations
WiMOD_SAP_LORAWAN_ProLink.h File Reference
`#include "WiMOD_SAP_LORAWAN.h"`
`#include "WiMOD_SAP_LORAWAN_ProLink_IDs.h"`
Include dependency graph for WiMOD_SAP_LORAWAN_ProLink.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Classes
class | WiMOD_SAP_LoRaWAN_ProLink
| Implementation for the ServiceAccessPoint LoRaWAN (End Node Modem firmware only) More...

## Typedefs
typedef enum TProLinkLoRaWANregion | TProLinkLoRaWANregion
| LoRaWAN Region support.
typedef void(* | TResetDevNonceIndicationCallback) (void)
typedef void(* | TLinkDisconnectIndicationCallback) (void)
typedef void(* | TNwkDeviceTimeAnsIndicationCallback) (TWiMODLR_HCIMessage &rxMsg)
typedef void(* | TMCastDataIndicationCallback) (TWiMODLR_HCIMessage &rxMsg)
typedef void(* | TMCastInvalidDataIndicationCallback) (TWiMODLR_HCIMessage &rxMsg)

## Enumerations
enum | TProLinkLoRaWANregion { ProLink_LoRaWAN_Region_EU868, ProLink_LoRaWAN_Region_US915, ProLink_LoRaWAN_Region_IN865, ProLink_LoRaWAN_Region_AU915, ProLink_LoRaWAN_Region_AS923, ProLink_LoRaWAN_Region_RU868, ProLink_LoRaWAN_Region_proprietary_WW2G4 }
| LoRaWAN Region support. More...

## Typedef Documentation

## ◆ TLinkDisconnectIndicationCallback

typedef void(* TLinkDisconnectIndicationCallback) (void)

Type definition for a 'link disconnect' indication callback function

## ◆ TMCastDataIndicationCallback

typedef void(* TMCastDataIndicationCallback) (TWiMODLR_HCIMessage &rxMsg)

Type definition for a 'Multicast RX Data' indication callback function

## ◆ TMCastInvalidDataIndicationCallback

typedef void(* TMCastInvalidDataIndicationCallback) (TWiMODLR_HCIMessage &rxMsg)

Type definition for a 'Multicast RX Invalid Data' indication callback function

## ◆ TNwkDeviceTimeAnsIndicationCallback

typedef void(* TNwkDeviceTimeAnsIndicationCallback) (TWiMODLR_HCIMessage &rxMsg)

Type definition for a 'network-device-time answer' indication callback function

## ◆ TResetDevNonceIndicationCallback

typedef void(* TResetDevNonceIndicationCallback) (void)

Type definition for a 'join tx' indication callback function

## Enumeration Type Documentation

## ◆ TProLinkLoRaWANregion

enum TProLinkLoRaWANregion

LoRaWAN Region support.

Enumerator
ProLink_LoRaWAN_Region_EU868 | regional settings for EU 868 MHz
ProLink_LoRaWAN_Region_US915 | regional settings for US 915 MHz
ProLink_LoRaWAN_Region_IN865 | regional settings for India 865 MHz
ProLink_LoRaWAN_Region_AU915 | regional settings for Australia 915 MHz
ProLink_LoRaWAN_Region_AS923 | regional settings for Asia 923 MHz
ProLink_LoRaWAN_Region_RU868 | regional settings for Russia 868 MHz